From e39d70502f7a981f821243160501303b7ee26d52 Mon Sep 17 00:00:00 2001
From: Mark Weiman <mark.weiman@markzz.com>
Date: Sat, 29 Jul 2017 09:15:32 -0400
Subject: [PATCH 3/6] pci: Enable overrides for missing ACS capabilities
 (4.12+)
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This an updated version of Alex Williamson's patch from:
https://lkml.org/lkml/2013/5/30/513

Original commit message follows:
PCIe ACS (Access Control Services) is the PCIe 2.0+ feature that
allows us to control whether transactions are allowed to be redirected
in various subnodes of a PCIe topology.  For instance, if two
endpoints are below a root port or downsteam switch port, the
downstream port may optionally redirect transactions between the
devices, bypassing upstream devices.  The same can happen internally
on multifunction devices.  The transaction may never be visible to the
upstream devices.

One upstream device that we particularly care about is the IOMMU.  If
a redirection occurs in the topology below the IOMMU, then the IOMMU
cannot provide isolation between devices.  This is why the PCIe spec
encourages topologies to include ACS support.  Without it, we have to
assume peer-to-peer DMA within a hierarchy can bypass IOMMU isolation.

Unfortunately, far too many topologies do not support ACS to make this
a steadfast requirement.  Even the latest chipsets from Intel are only
sporadically supporting ACS.  We have trouble getting interconnect
vendors to include the PCIe spec required PCIe capability, let alone
suggested features.

Therefore, we need to add some flexibility.  The pcie_acs_override=
boot option lets users opt-in specific devices or sets of devices to
assume ACS support.  The "downstream" option assumes full ACS support
on root ports and downstream switch ports.  The "multifunction"
option assumes the subset of ACS features available on multifunction
endpoints and upstream switch ports are supported.  The "id:nnnn:nnnn"
option enables ACS support on devices matching the provided vendor
and device IDs, allowing more strategic ACS overrides.  These options
may be combined in any order.  A maximum of 16 id specific overrides
are available.  It's suggested to use the most limited set of options
necessary to avoid completely disabling ACS across the topology.
Note to hardware vendors, we have facilities to permanently quirk
specific devices which enforce isolation but not provide an ACS
capability.  Please contact me to have your devices added and save
your customers the hassle of this boot option.

Signed-off-by: Fabian Grünbichler <f.gruenbichler@proxmox.com>
---
 Documentation/admin-guide/kernel-parameters.txt |   9 +++
 drivers/pci/quirks.c                            | 102 ++++++++++++++++++++++++
 2 files changed, 111 insertions(+)

diff --git a/Documentation/admin-guide/kernel-parameters.txt b/Documentation/admin-guide/kernel-parameters.txt
index f8ce2089146c..d4ace16bd59a 100644
--- a/Documentation/admin-guide/kernel-parameters.txt
+++ b/Documentation/admin-guide/kernel-parameters.txt
@@ -2918,6 +2918,15 @@
 		nomsi		[MSI] If the PCI_MSI kernel config parameter is
 				enabled, this kernel boot option can be used to
 				disable the use of MSI interrupts system-wide.
+		pci_acs_override =
+					[PCIE] Override missing PCIe ACS support for:
+				downstream
+					All downstream ports - full ACS capabilities
+				multfunction
+					All multifunction devices - multifunction ACS subset
+				id:nnnn:nnnn
+					Specfic device - full ACS capabilities
+					Specified as vid:did (vendor/device ID) in hex
 		noioapicquirk	[APIC] Disable all boot interrupt quirks.
 				Safety option to keep boot IRQs enabled. This
 				should never be necessary.
diff --git a/drivers/pci/quirks.c b/drivers/pci/quirks.c
index b7832fd4dbf4..f128ca4aea2b 100644
--- a/drivers/pci/quirks.c
+++ b/drivers/pci/quirks.c
@@ -3687,6 +3687,107 @@ static int __init pci_apply_final_quirks(void)
 
 fs_initcall_sync(pci_apply_final_quirks);
 
+static bool acs_on_downstream;
+static bool acs_on_multifunction;
+
+#define NUM_ACS_IDS 16
+struct acs_on_id {
+	unsigned short vendor;
+	unsigned short device;
+};
+static struct acs_on_id acs_on_ids[NUM_ACS_IDS];
+static u8 max_acs_id;
+
+static __init int pcie_acs_override_setup(char *p)
+{
+	if (!p)
+		return -EINVAL;
+
+	while (*p) {
+		if (!strncmp(p, "downstream", 10))
+			acs_on_downstream = true;
+		if (!strncmp(p, "multifunction", 13))
+			acs_on_multifunction = true;
+		if (!strncmp(p, "id:", 3)) {
+			char opt[5];
+			int ret;
+			long val;
+
+			if (max_acs_id >= NUM_ACS_IDS - 1) {
+				pr_warn("Out of PCIe ACS override slots (%d)\n",
+						NUM_ACS_IDS);
+				goto next;
+			}
+
+			p += 3;
+			snprintf(opt, 5, "%s", p);
+			ret = kstrtol(opt, 16, &val);
+			if (ret) {
+				pr_warn("PCIe ACS ID parse error %d\n", ret);
+				goto next;
+			}
+			acs_on_ids[max_acs_id].vendor = val;
+
+			p += strcspn(p, ":");
+			if (*p != ':') {
+				pr_warn("PCIe ACS invalid ID\n");
+				goto next;
+			}
+
+			p++;
+			snprintf(opt, 5, "%s", p);
+			ret = kstrtol(opt, 16, &val);
+			if (ret) {
+				pr_warn("PCIe ACS ID parse error %d\n", ret);
+				goto next;
+			}
+			acs_on_ids[max_acs_id].device = val;
+			max_acs_id++;
+		}
+next:
+		p += strcspn(p, ",");
+		if (*p == ',')
+			p++;
+	}
+
+	if (acs_on_downstream || acs_on_multifunction || max_acs_id)
+		pr_warn("Warning: PCIe ACS overrides enabled; This may allow non-IOMMU protected peer-to-peer DMA\n");
+
+	return 0;
+}
+early_param("pcie_acs_override", pcie_acs_override_setup);
+
+static int pcie_acs_overrides(struct pci_dev *dev, u16 acs_flags)
+{
+	int i;
+
+	/* Never override ACS for legacy devices or devices with ACS caps */
+	if (!pci_is_pcie(dev) ||
+		pci_find_ext_capability(dev, PCI_EXT_CAP_ID_ACS))
+			return -ENOTTY;
+
+	for (i = 0; i < max_acs_id; i++)
+		if (acs_on_ids[i].vendor == dev->vendor &&
+			acs_on_ids[i].device == dev->device)
+				return 1;
+
+	switch (pci_pcie_type(dev)) {
+	case PCI_EXP_TYPE_DOWNSTREAM:
+	case PCI_EXP_TYPE_ROOT_PORT:
+		if (acs_on_downstream)
+			return 1;
+		break;
+	case PCI_EXP_TYPE_ENDPOINT:
+	case PCI_EXP_TYPE_UPSTREAM:
+	case PCI_EXP_TYPE_LEG_END:
+	case PCI_EXP_TYPE_RC_END:
+		if (acs_on_multifunction && dev->multifunction)
+			return 1;
+	}
+
+	return -ENOTTY;
+}
+
 /*
  * Following are device-specific reset methods which can be used to
  * reset a single function if other methods (e.g. FLR, PM D0->D3) are
@@ -4490,6 +4591,7 @@ static const struct pci_dev_acs_enabled {
 	{ 0x10df, 0x720, pci_quirk_mf_endpoint_acs }, /* Emulex Skyhawk-R */
 	/* Cavium ThunderX */
 	{ PCI_VENDOR_ID_CAVIUM, PCI_ANY_ID, pci_quirk_cavium_acs },
+	{ PCI_ANY_ID, PCI_ANY_ID, pcie_acs_overrides },
 	{ 0 }
 };
 
-- 
2.11.0

