 src/{ixgbe_ptp.c.orig => ixgbe_ptp.c} | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/src/ixgbe_ptp.c.orig b/src/ixgbe_ptp.c
index fb832f0..b868c68 100644
--- a/src/ixgbe_ptp.c.orig
+++ b/src/ixgbe_ptp.c
@@ -244,7 +244,7 @@ static void ixgbe_ptp_setup_sdp_X540(struct ixgbe_adapter *adapter)
  * result of SYSTIME is 32bits of "billions of cycles" and 32 bits of
  * "cycles", rather than seconds and nanoseconds.
  */
-static cycle_t ixgbe_ptp_read_X550(const struct cyclecounter *hw_cc) {
+static u64 ixgbe_ptp_read_X550(const struct cyclecounter *hw_cc) {
 	struct ixgbe_adapter *adapter =
 		container_of(hw_cc, struct ixgbe_adapter, hw_cc);
 	struct ixgbe_hw *hw = &adapter->hw;
@@ -280,7 +280,7 @@ static cycle_t ixgbe_ptp_read_X550(const struct cyclecounter *hw_cc) {
  * cyclecounter structure used to construct a ns counter from the
  * arbitrary fixed point registers
  */
-static cycle_t ixgbe_ptp_read_82599(const struct cyclecounter *hw_cc)
+static u64 ixgbe_ptp_read_82599(const struct cyclecounter *hw_cc)
 {
 	struct ixgbe_adapter *adapter =
 		container_of(hw_cc, struct ixgbe_adapter, hw_cc);
