From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Tim Chen <tim.c.chen@linux.intel.com>
Date: Fri, 20 Oct 2017 12:56:29 -0700
Subject: [PATCH] x86/mm: Set IBPB upon context switch
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

CVE-2017-5753
CVE-2017-5715

Set IBPB on context switch with changing of page table.

Signed-off-by: Tim Chen <tim.c.chen@linux.intel.com>
Signed-off-by: Andy Whitcroft <apw@canonical.com>
Signed-off-by: Kleber Sacilotto de Souza <kleber.souza@canonical.com>
(cherry picked from commit a3320203792b633fb96df5d0bbfb7036129b78e2)
Signed-off-by: Fabian Grünbichler <f.gruenbichler@proxmox.com>
---
 arch/x86/mm/tlb.c | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/arch/x86/mm/tlb.c b/arch/x86/mm/tlb.c
index 06f3854d0a4f..bb3ded3a4e5f 100644
--- a/arch/x86/mm/tlb.c
+++ b/arch/x86/mm/tlb.c
@@ -12,6 +12,7 @@
 #include <asm/cache.h>
 #include <asm/apic.h>
 #include <asm/uv/uv.h>
+#include <asm/microcode.h>
 #include <linux/debugfs.h>
 
 /*
@@ -218,6 +219,9 @@ void switch_mm_irqs_off(struct mm_struct *prev, struct mm_struct *next,
 		u16 new_asid;
 		bool need_flush;
 
+		if (boot_cpu_has(X86_FEATURE_SPEC_CTRL))
+			native_wrmsrl(MSR_IA32_PRED_CMD, FEATURE_SET_IBPB);
+
 		if (IS_ENABLED(CONFIG_VMAP_STACK)) {
 			/*
 			 * If our current stack is in vmalloc space and isn't
-- 
2.14.2

