From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Andy Lutomirski <luto@kernel.org>
Date: Mon, 4 Dec 2017 15:07:19 +0100
Subject: [PATCH] x86/entry: Move SYSENTER_stack to the beginning of struct
 tss_struct
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

CVE-2017-5754

SYSENTER_stack should have reliable overflow detection, which
means that it needs to be at the bottom of a page, not the top.
Move it to the beginning of struct tss_struct and page-align it.

Also add an assertion to make sure that the fixed hardware TSS
doesn't cross a page boundary.

Signed-off-by: Andy Lutomirski <luto@kernel.org>
Signed-off-by: Thomas Gleixner <tglx@linutronix.de>
Reviewed-by: Thomas Gleixner <tglx@linutronix.de>
Reviewed-by: Borislav Petkov <bp@suse.de>
Cc: Boris Ostrovsky <boris.ostrovsky@oracle.com>
Cc: Borislav Petkov <bp@alien8.de>
Cc: Borislav Petkov <bpetkov@suse.de>
Cc: Brian Gerst <brgerst@gmail.com>
Cc: Dave Hansen <dave.hansen@intel.com>
Cc: Dave Hansen <dave.hansen@linux.intel.com>
Cc: David Laight <David.Laight@aculab.com>
Cc: Denys Vlasenko <dvlasenk@redhat.com>
Cc: Eduardo Valentin <eduval@amazon.com>
Cc: Greg KH <gregkh@linuxfoundation.org>
Cc: H. Peter Anvin <hpa@zytor.com>
Cc: Josh Poimboeuf <jpoimboe@redhat.com>
Cc: Juergen Gross <jgross@suse.com>
Cc: Linus Torvalds <torvalds@linux-foundation.org>
Cc: Peter Zijlstra <peterz@infradead.org>
Cc: Rik van Riel <riel@redhat.com>
Cc: Will Deacon <will.deacon@arm.com>
Cc: aliguori@amazon.com
Cc: daniel.gruss@iaik.tugraz.at
Cc: hughd@google.com
Cc: keescook@google.com
Link: https://lkml.kernel.org/r/20171204150605.881827433@linutronix.de
Signed-off-by: Ingo Molnar <mingo@kernel.org>
(cherry picked from commit 1a935bc3d4ea61556461a9e92a68ca3556232efd)
Signed-off-by: Andy Whitcroft <apw@canonical.com>
Signed-off-by: Kleber Sacilotto de Souza <kleber.souza@canonical.com>
(cherry picked from commit 57d6cfd9e7d015aabbed6d0b50e7d2525b3c86c2)
Signed-off-by: Fabian Grünbichler <f.gruenbichler@proxmox.com>
---
 arch/x86/include/asm/processor.h | 21 ++++++++++++---------
 arch/x86/kernel/cpu/common.c     | 21 +++++++++++++++++++++
 2 files changed, 33 insertions(+), 9 deletions(-)

diff --git a/arch/x86/include/asm/processor.h b/arch/x86/include/asm/processor.h
index 78123abdb046..55885465c3a7 100644
--- a/arch/x86/include/asm/processor.h
+++ b/arch/x86/include/asm/processor.h
@@ -326,7 +326,16 @@ struct x86_hw_tss {
 
 struct tss_struct {
 	/*
-	 * The hardware state:
+	 * Space for the temporary SYSENTER stack, used for SYSENTER
+	 * and the entry trampoline as well.
+	 */
+	unsigned long		SYSENTER_stack_canary;
+	unsigned long		SYSENTER_stack[64];
+
+	/*
+	 * The fixed hardware portion.  This must not cross a page boundary
+	 * at risk of violating the SDM's advice and potentially triggering
+	 * errata.
 	 */
 	struct x86_hw_tss	x86_tss;
 
@@ -337,15 +346,9 @@ struct tss_struct {
 	 * be within the limit.
 	 */
 	unsigned long		io_bitmap[IO_BITMAP_LONGS + 1];
+} __aligned(PAGE_SIZE);
 
-	/*
-	 * Space for the temporary SYSENTER stack.
-	 */
-	unsigned long		SYSENTER_stack_canary;
-	unsigned long		SYSENTER_stack[64];
-} ____cacheline_aligned;
-
-DECLARE_PER_CPU_SHARED_ALIGNED(struct tss_struct, cpu_tss);
+DECLARE_PER_CPU_PAGE_ALIGNED(struct tss_struct, cpu_tss);
 
 /*
  * sizeof(unsigned long) coming from an extra "long" at the end
diff --git a/arch/x86/kernel/cpu/common.c b/arch/x86/kernel/cpu/common.c
index e526d82b546c..e61eff11f562 100644
--- a/arch/x86/kernel/cpu/common.c
+++ b/arch/x86/kernel/cpu/common.c
@@ -487,6 +487,27 @@ static inline void setup_cpu_entry_area(int cpu)
 #endif
 
 	__set_fixmap(get_cpu_entry_area_index(cpu, gdt), get_cpu_gdt_paddr(cpu), gdt_prot);
+
+	/*
+	 * The Intel SDM says (Volume 3, 7.2.1):
+	 *
+	 *  Avoid placing a page boundary in the part of the TSS that the
+	 *  processor reads during a task switch (the first 104 bytes). The
+	 *  processor may not correctly perform address translations if a
+	 *  boundary occurs in this area. During a task switch, the processor
+	 *  reads and writes into the first 104 bytes of each TSS (using
+	 *  contiguous physical addresses beginning with the physical address
+	 *  of the first byte of the TSS). So, after TSS access begins, if
+	 *  part of the 104 bytes is not physically contiguous, the processor
+	 *  will access incorrect information without generating a page-fault
+	 *  exception.
+	 *
+	 * There are also a lot of errata involving the TSS spanning a page
+	 * boundary.  Assert that we're not doing that.
+	 */
+	BUILD_BUG_ON((offsetof(struct tss_struct, x86_tss) ^
+		      offsetofend(struct tss_struct, x86_tss)) & PAGE_MASK);
+
 }
 
 /* Load the original GDT from the per-cpu structure */
-- 
2.14.2

