From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Ingo Molnar <mingo@kernel.org>
Date: Tue, 31 Oct 2017 13:17:22 +0100
Subject: [PATCH] x86/cpufeatures: Re-tabulate the X86_FEATURE definitions
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

CVE-2017-5754

Over the years asm/cpufeatures.h has become somewhat of a mess: the original
tabulation style was too narrow, while x86 feature names also kept growing
in length, creating frequent field width overflows.

Re-tabulate it to make it wider and easier to read/modify. Also harmonize
the tabulation of the other defines in this file to match it.

Cc: Andrew Morton <akpm@linux-foundation.org>
Cc: Andy Lutomirski <luto@amacapital.net>
Cc: Andy Lutomirski <luto@kernel.org>
Cc: Borislav Petkov <bp@alien8.de>
Cc: Brian Gerst <brgerst@gmail.com>
Cc: Denys Vlasenko <dvlasenk@redhat.com>
Cc: Josh Poimboeuf <jpoimboe@redhat.com>
Cc: Linus Torvalds <torvalds@linux-foundation.org>
Cc: Peter Zijlstra <peterz@infradead.org>
Cc: Thomas Gleixner <tglx@linutronix.de>
Link: http://lkml.kernel.org/r/20171031121723.28524-3-mingo@kernel.org
Signed-off-by: Ingo Molnar <mingo@kernel.org>
(backported from commit acbc845ffefd9fb70466182cd8555a26189462b2)
Signed-off-by: Andy Whitcroft <apw@canonical.com>
Signed-off-by: Kleber Sacilotto de Souza <kleber.souza@canonical.com>
(cherry picked from commit df7c6e7b62274889a028357a579acfb2215c3f98)
Signed-off-by: Fabian Grünbichler <f.gruenbichler@proxmox.com>
---
 arch/x86/include/asm/cpufeatures.h | 506 +++++++++++++++++++------------------
 1 file changed, 254 insertions(+), 252 deletions(-)

diff --git a/arch/x86/include/asm/cpufeatures.h b/arch/x86/include/asm/cpufeatures.h
index c465bd6613ed..a021b0756af6 100644
--- a/arch/x86/include/asm/cpufeatures.h
+++ b/arch/x86/include/asm/cpufeatures.h
@@ -12,8 +12,8 @@
 /*
  * Defines x86 CPU feature bits
  */
-#define NCAPINTS	18	/* N 32-bit words worth of info */
-#define NBUGINTS	1	/* N 32-bit bug flags */
+#define NCAPINTS			18	   /* N 32-bit words worth of info */
+#define NBUGINTS			1	   /* N 32-bit bug flags */
 
 /*
  * Note: If the comment begins with a quoted string, that string is used
@@ -27,163 +27,163 @@
  */
 
 /* Intel-defined CPU features, CPUID level 0x00000001 (edx), word 0 */
-#define X86_FEATURE_FPU		( 0*32+ 0) /* Onboard FPU */
-#define X86_FEATURE_VME		( 0*32+ 1) /* Virtual Mode Extensions */
-#define X86_FEATURE_DE		( 0*32+ 2) /* Debugging Extensions */
-#define X86_FEATURE_PSE		( 0*32+ 3) /* Page Size Extensions */
-#define X86_FEATURE_TSC		( 0*32+ 4) /* Time Stamp Counter */
-#define X86_FEATURE_MSR		( 0*32+ 5) /* Model-Specific Registers */
-#define X86_FEATURE_PAE		( 0*32+ 6) /* Physical Address Extensions */
-#define X86_FEATURE_MCE		( 0*32+ 7) /* Machine Check Exception */
-#define X86_FEATURE_CX8		( 0*32+ 8) /* CMPXCHG8 instruction */
-#define X86_FEATURE_APIC	( 0*32+ 9) /* Onboard APIC */
-#define X86_FEATURE_SEP		( 0*32+11) /* SYSENTER/SYSEXIT */
-#define X86_FEATURE_MTRR	( 0*32+12) /* Memory Type Range Registers */
-#define X86_FEATURE_PGE		( 0*32+13) /* Page Global Enable */
-#define X86_FEATURE_MCA		( 0*32+14) /* Machine Check Architecture */
-#define X86_FEATURE_CMOV	( 0*32+15) /* CMOV instructions */
+#define X86_FEATURE_FPU			( 0*32+ 0) /* Onboard FPU */
+#define X86_FEATURE_VME			( 0*32+ 1) /* Virtual Mode Extensions */
+#define X86_FEATURE_DE			( 0*32+ 2) /* Debugging Extensions */
+#define X86_FEATURE_PSE			( 0*32+ 3) /* Page Size Extensions */
+#define X86_FEATURE_TSC			( 0*32+ 4) /* Time Stamp Counter */
+#define X86_FEATURE_MSR			( 0*32+ 5) /* Model-Specific Registers */
+#define X86_FEATURE_PAE			( 0*32+ 6) /* Physical Address Extensions */
+#define X86_FEATURE_MCE			( 0*32+ 7) /* Machine Check Exception */
+#define X86_FEATURE_CX8			( 0*32+ 8) /* CMPXCHG8 instruction */
+#define X86_FEATURE_APIC		( 0*32+ 9) /* Onboard APIC */
+#define X86_FEATURE_SEP			( 0*32+11) /* SYSENTER/SYSEXIT */
+#define X86_FEATURE_MTRR		( 0*32+12) /* Memory Type Range Registers */
+#define X86_FEATURE_PGE			( 0*32+13) /* Page Global Enable */
+#define X86_FEATURE_MCA			( 0*32+14) /* Machine Check Architecture */
+#define X86_FEATURE_CMOV		( 0*32+15) /* CMOV instructions */
 					  /* (plus FCMOVcc, FCOMI with FPU) */
-#define X86_FEATURE_PAT		( 0*32+16) /* Page Attribute Table */
-#define X86_FEATURE_PSE36	( 0*32+17) /* 36-bit PSEs */
-#define X86_FEATURE_PN		( 0*32+18) /* Processor serial number */
-#define X86_FEATURE_CLFLUSH	( 0*32+19) /* CLFLUSH instruction */
-#define X86_FEATURE_DS		( 0*32+21) /* "dts" Debug Store */
-#define X86_FEATURE_ACPI	( 0*32+22) /* ACPI via MSR */
-#define X86_FEATURE_MMX		( 0*32+23) /* Multimedia Extensions */
-#define X86_FEATURE_FXSR	( 0*32+24) /* FXSAVE/FXRSTOR, CR4.OSFXSR */
-#define X86_FEATURE_XMM		( 0*32+25) /* "sse" */
-#define X86_FEATURE_XMM2	( 0*32+26) /* "sse2" */
-#define X86_FEATURE_SELFSNOOP	( 0*32+27) /* "ss" CPU self snoop */
-#define X86_FEATURE_HT		( 0*32+28) /* Hyper-Threading */
-#define X86_FEATURE_ACC		( 0*32+29) /* "tm" Automatic clock control */
-#define X86_FEATURE_IA64	( 0*32+30) /* IA-64 processor */
-#define X86_FEATURE_PBE		( 0*32+31) /* Pending Break Enable */
+#define X86_FEATURE_PAT			( 0*32+16) /* Page Attribute Table */
+#define X86_FEATURE_PSE36		( 0*32+17) /* 36-bit PSEs */
+#define X86_FEATURE_PN			( 0*32+18) /* Processor serial number */
+#define X86_FEATURE_CLFLUSH		( 0*32+19) /* CLFLUSH instruction */
+#define X86_FEATURE_DS			( 0*32+21) /* "dts" Debug Store */
+#define X86_FEATURE_ACPI		( 0*32+22) /* ACPI via MSR */
+#define X86_FEATURE_MMX			( 0*32+23) /* Multimedia Extensions */
+#define X86_FEATURE_FXSR		( 0*32+24) /* FXSAVE/FXRSTOR, CR4.OSFXSR */
+#define X86_FEATURE_XMM			( 0*32+25) /* "sse" */
+#define X86_FEATURE_XMM2		( 0*32+26) /* "sse2" */
+#define X86_FEATURE_SELFSNOOP		( 0*32+27) /* "ss" CPU self snoop */
+#define X86_FEATURE_HT			( 0*32+28) /* Hyper-Threading */
+#define X86_FEATURE_ACC			( 0*32+29) /* "tm" Automatic clock control */
+#define X86_FEATURE_IA64		( 0*32+30) /* IA-64 processor */
+#define X86_FEATURE_PBE			( 0*32+31) /* Pending Break Enable */
 
 /* AMD-defined CPU features, CPUID level 0x80000001, word 1 */
 /* Don't duplicate feature flags which are redundant with Intel! */
-#define X86_FEATURE_SYSCALL	( 1*32+11) /* SYSCALL/SYSRET */
-#define X86_FEATURE_MP		( 1*32+19) /* MP Capable. */
-#define X86_FEATURE_NX		( 1*32+20) /* Execute Disable */
-#define X86_FEATURE_MMXEXT	( 1*32+22) /* AMD MMX extensions */
-#define X86_FEATURE_FXSR_OPT	( 1*32+25) /* FXSAVE/FXRSTOR optimizations */
-#define X86_FEATURE_GBPAGES	( 1*32+26) /* "pdpe1gb" GB pages */
-#define X86_FEATURE_RDTSCP	( 1*32+27) /* RDTSCP */
-#define X86_FEATURE_LM		( 1*32+29) /* Long Mode (x86-64) */
-#define X86_FEATURE_3DNOWEXT	( 1*32+30) /* AMD 3DNow! extensions */
-#define X86_FEATURE_3DNOW	( 1*32+31) /* 3DNow! */
+#define X86_FEATURE_SYSCALL		( 1*32+11) /* SYSCALL/SYSRET */
+#define X86_FEATURE_MP			( 1*32+19) /* MP Capable. */
+#define X86_FEATURE_NX			( 1*32+20) /* Execute Disable */
+#define X86_FEATURE_MMXEXT		( 1*32+22) /* AMD MMX extensions */
+#define X86_FEATURE_FXSR_OPT		( 1*32+25) /* FXSAVE/FXRSTOR optimizations */
+#define X86_FEATURE_GBPAGES		( 1*32+26) /* "pdpe1gb" GB pages */
+#define X86_FEATURE_RDTSCP		( 1*32+27) /* RDTSCP */
+#define X86_FEATURE_LM			( 1*32+29) /* Long Mode (x86-64) */
+#define X86_FEATURE_3DNOWEXT		( 1*32+30) /* AMD 3DNow! extensions */
+#define X86_FEATURE_3DNOW		( 1*32+31) /* 3DNow! */
 
 /* Transmeta-defined CPU features, CPUID level 0x80860001, word 2 */
-#define X86_FEATURE_RECOVERY	( 2*32+ 0) /* CPU in recovery mode */
-#define X86_FEATURE_LONGRUN	( 2*32+ 1) /* Longrun power control */
-#define X86_FEATURE_LRTI	( 2*32+ 3) /* LongRun table interface */
+#define X86_FEATURE_RECOVERY		( 2*32+ 0) /* CPU in recovery mode */
+#define X86_FEATURE_LONGRUN		( 2*32+ 1) /* Longrun power control */
+#define X86_FEATURE_LRTI		( 2*32+ 3) /* LongRun table interface */
 
 /* Other features, Linux-defined mapping, word 3 */
 /* This range is used for feature bits which conflict or are synthesized */
-#define X86_FEATURE_CXMMX	( 3*32+ 0) /* Cyrix MMX extensions */
-#define X86_FEATURE_K6_MTRR	( 3*32+ 1) /* AMD K6 nonstandard MTRRs */
-#define X86_FEATURE_CYRIX_ARR	( 3*32+ 2) /* Cyrix ARRs (= MTRRs) */
-#define X86_FEATURE_CENTAUR_MCR	( 3*32+ 3) /* Centaur MCRs (= MTRRs) */
+#define X86_FEATURE_CXMMX		( 3*32+ 0) /* Cyrix MMX extensions */
+#define X86_FEATURE_K6_MTRR		( 3*32+ 1) /* AMD K6 nonstandard MTRRs */
+#define X86_FEATURE_CYRIX_ARR		( 3*32+ 2) /* Cyrix ARRs (= MTRRs) */
+#define X86_FEATURE_CENTAUR_MCR		( 3*32+ 3) /* Centaur MCRs (= MTRRs) */
 /* cpu types for specific tunings: */
-#define X86_FEATURE_K8		( 3*32+ 4) /* "" Opteron, Athlon64 */
-#define X86_FEATURE_K7		( 3*32+ 5) /* "" Athlon */
-#define X86_FEATURE_P3		( 3*32+ 6) /* "" P3 */
-#define X86_FEATURE_P4		( 3*32+ 7) /* "" P4 */
-#define X86_FEATURE_CONSTANT_TSC ( 3*32+ 8) /* TSC ticks at a constant rate */
-#define X86_FEATURE_UP		( 3*32+ 9) /* smp kernel running on up */
-#define X86_FEATURE_ART		( 3*32+10) /* Platform has always running timer (ART) */
-#define X86_FEATURE_ARCH_PERFMON ( 3*32+11) /* Intel Architectural PerfMon */
-#define X86_FEATURE_PEBS	( 3*32+12) /* Precise-Event Based Sampling */
-#define X86_FEATURE_BTS		( 3*32+13) /* Branch Trace Store */
-#define X86_FEATURE_SYSCALL32	( 3*32+14) /* "" syscall in ia32 userspace */
-#define X86_FEATURE_SYSENTER32	( 3*32+15) /* "" sysenter in ia32 userspace */
-#define X86_FEATURE_REP_GOOD	( 3*32+16) /* rep microcode works well */
-#define X86_FEATURE_MFENCE_RDTSC ( 3*32+17) /* "" Mfence synchronizes RDTSC */
-#define X86_FEATURE_LFENCE_RDTSC ( 3*32+18) /* "" Lfence synchronizes RDTSC */
-#define X86_FEATURE_ACC_POWER	( 3*32+19) /* AMD Accumulated Power Mechanism */
-#define X86_FEATURE_NOPL	( 3*32+20) /* The NOPL (0F 1F) instructions */
-#define X86_FEATURE_ALWAYS	( 3*32+21) /* "" Always-present feature */
-#define X86_FEATURE_XTOPOLOGY	( 3*32+22) /* cpu topology enum extensions */
-#define X86_FEATURE_TSC_RELIABLE ( 3*32+23) /* TSC is known to be reliable */
-#define X86_FEATURE_NONSTOP_TSC	( 3*32+24) /* TSC does not stop in C states */
-#define X86_FEATURE_CPUID	( 3*32+25) /* CPU has CPUID instruction itself */
-#define X86_FEATURE_EXTD_APICID	( 3*32+26) /* has extended APICID (8 bits) */
-#define X86_FEATURE_AMD_DCM     ( 3*32+27) /* multi-node processor */
-#define X86_FEATURE_APERFMPERF	( 3*32+28) /* APERFMPERF */
-#define X86_FEATURE_NONSTOP_TSC_S3 ( 3*32+30) /* TSC doesn't stop in S3 state */
-#define X86_FEATURE_TSC_KNOWN_FREQ ( 3*32+31) /* TSC has known frequency */
+#define X86_FEATURE_K8			( 3*32+ 4) /* "" Opteron, Athlon64 */
+#define X86_FEATURE_K7			( 3*32+ 5) /* "" Athlon */
+#define X86_FEATURE_P3			( 3*32+ 6) /* "" P3 */
+#define X86_FEATURE_P4			( 3*32+ 7) /* "" P4 */
+#define X86_FEATURE_CONSTANT_TSC	( 3*32+ 8) /* TSC ticks at a constant rate */
+#define X86_FEATURE_UP			( 3*32+ 9) /* smp kernel running on up */
+#define X86_FEATURE_ART			( 3*32+10) /* Platform has always running timer (ART) */
+#define X86_FEATURE_ARCH_PERFMON	( 3*32+11) /* Intel Architectural PerfMon */
+#define X86_FEATURE_PEBS		( 3*32+12) /* Precise-Event Based Sampling */
+#define X86_FEATURE_BTS			( 3*32+13) /* Branch Trace Store */
+#define X86_FEATURE_SYSCALL32		( 3*32+14) /* "" syscall in ia32 userspace */
+#define X86_FEATURE_SYSENTER32		( 3*32+15) /* "" sysenter in ia32 userspace */
+#define X86_FEATURE_REP_GOOD		( 3*32+16) /* rep microcode works well */
+#define X86_FEATURE_MFENCE_RDTSC	( 3*32+17) /* "" Mfence synchronizes RDTSC */
+#define X86_FEATURE_LFENCE_RDTSC	( 3*32+18) /* "" Lfence synchronizes RDTSC */
+#define X86_FEATURE_ACC_POWER		( 3*32+19) /* AMD Accumulated Power Mechanism */
+#define X86_FEATURE_NOPL		( 3*32+20) /* The NOPL (0F 1F) instructions */
+#define X86_FEATURE_ALWAYS		( 3*32+21) /* "" Always-present feature */
+#define X86_FEATURE_XTOPOLOGY		( 3*32+22) /* cpu topology enum extensions */
+#define X86_FEATURE_TSC_RELIABLE	( 3*32+23) /* TSC is known to be reliable */
+#define X86_FEATURE_NONSTOP_TSC		( 3*32+24) /* TSC does not stop in C states */
+#define X86_FEATURE_CPUID		( 3*32+25) /* CPU has CPUID instruction itself */
+#define X86_FEATURE_EXTD_APICID		( 3*32+26) /* has extended APICID (8 bits) */
+#define X86_FEATURE_AMD_DCM		( 3*32+27) /* multi-node processor */
+#define X86_FEATURE_APERFMPERF		( 3*32+28) /* APERFMPERF */
+#define X86_FEATURE_NONSTOP_TSC_S3	( 3*32+30) /* TSC doesn't stop in S3 state */
+#define X86_FEATURE_TSC_KNOWN_FREQ	( 3*32+31) /* TSC has known frequency */
 
 /* Intel-defined CPU features, CPUID level 0x00000001 (ecx), word 4 */
-#define X86_FEATURE_XMM3	( 4*32+ 0) /* "pni" SSE-3 */
-#define X86_FEATURE_PCLMULQDQ	( 4*32+ 1) /* PCLMULQDQ instruction */
-#define X86_FEATURE_DTES64	( 4*32+ 2) /* 64-bit Debug Store */
-#define X86_FEATURE_MWAIT	( 4*32+ 3) /* "monitor" Monitor/Mwait support */
-#define X86_FEATURE_DSCPL	( 4*32+ 4) /* "ds_cpl" CPL Qual. Debug Store */
-#define X86_FEATURE_VMX		( 4*32+ 5) /* Hardware virtualization */
-#define X86_FEATURE_SMX		( 4*32+ 6) /* Safer mode */
-#define X86_FEATURE_EST		( 4*32+ 7) /* Enhanced SpeedStep */
-#define X86_FEATURE_TM2		( 4*32+ 8) /* Thermal Monitor 2 */
-#define X86_FEATURE_SSSE3	( 4*32+ 9) /* Supplemental SSE-3 */
-#define X86_FEATURE_CID		( 4*32+10) /* Context ID */
-#define X86_FEATURE_SDBG	( 4*32+11) /* Silicon Debug */
-#define X86_FEATURE_FMA		( 4*32+12) /* Fused multiply-add */
-#define X86_FEATURE_CX16	( 4*32+13) /* CMPXCHG16B */
-#define X86_FEATURE_XTPR	( 4*32+14) /* Send Task Priority Messages */
-#define X86_FEATURE_PDCM	( 4*32+15) /* Performance Capabilities */
-#define X86_FEATURE_PCID	( 4*32+17) /* Process Context Identifiers */
-#define X86_FEATURE_DCA		( 4*32+18) /* Direct Cache Access */
-#define X86_FEATURE_XMM4_1	( 4*32+19) /* "sse4_1" SSE-4.1 */
-#define X86_FEATURE_XMM4_2	( 4*32+20) /* "sse4_2" SSE-4.2 */
-#define X86_FEATURE_X2APIC	( 4*32+21) /* x2APIC */
-#define X86_FEATURE_MOVBE	( 4*32+22) /* MOVBE instruction */
-#define X86_FEATURE_POPCNT      ( 4*32+23) /* POPCNT instruction */
+#define X86_FEATURE_XMM3		( 4*32+ 0) /* "pni" SSE-3 */
+#define X86_FEATURE_PCLMULQDQ		( 4*32+ 1) /* PCLMULQDQ instruction */
+#define X86_FEATURE_DTES64		( 4*32+ 2) /* 64-bit Debug Store */
+#define X86_FEATURE_MWAIT		( 4*32+ 3) /* "monitor" Monitor/Mwait support */
+#define X86_FEATURE_DSCPL		( 4*32+ 4) /* "ds_cpl" CPL Qual. Debug Store */
+#define X86_FEATURE_VMX			( 4*32+ 5) /* Hardware virtualization */
+#define X86_FEATURE_SMX			( 4*32+ 6) /* Safer mode */
+#define X86_FEATURE_EST			( 4*32+ 7) /* Enhanced SpeedStep */
+#define X86_FEATURE_TM2			( 4*32+ 8) /* Thermal Monitor 2 */
+#define X86_FEATURE_SSSE3		( 4*32+ 9) /* Supplemental SSE-3 */
+#define X86_FEATURE_CID			( 4*32+10) /* Context ID */
+#define X86_FEATURE_SDBG		( 4*32+11) /* Silicon Debug */
+#define X86_FEATURE_FMA			( 4*32+12) /* Fused multiply-add */
+#define X86_FEATURE_CX16		( 4*32+13) /* CMPXCHG16B */
+#define X86_FEATURE_XTPR		( 4*32+14) /* Send Task Priority Messages */
+#define X86_FEATURE_PDCM		( 4*32+15) /* Performance Capabilities */
+#define X86_FEATURE_PCID		( 4*32+17) /* Process Context Identifiers */
+#define X86_FEATURE_DCA			( 4*32+18) /* Direct Cache Access */
+#define X86_FEATURE_XMM4_1		( 4*32+19) /* "sse4_1" SSE-4.1 */
+#define X86_FEATURE_XMM4_2		( 4*32+20) /* "sse4_2" SSE-4.2 */
+#define X86_FEATURE_X2APIC		( 4*32+21) /* x2APIC */
+#define X86_FEATURE_MOVBE		( 4*32+22) /* MOVBE instruction */
+#define X86_FEATURE_POPCNT		( 4*32+23) /* POPCNT instruction */
 #define X86_FEATURE_TSC_DEADLINE_TIMER	( 4*32+24) /* Tsc deadline timer */
-#define X86_FEATURE_AES		( 4*32+25) /* AES instructions */
-#define X86_FEATURE_XSAVE	( 4*32+26) /* XSAVE/XRSTOR/XSETBV/XGETBV */
-#define X86_FEATURE_OSXSAVE	( 4*32+27) /* "" XSAVE enabled in the OS */
-#define X86_FEATURE_AVX		( 4*32+28) /* Advanced Vector Extensions */
-#define X86_FEATURE_F16C	( 4*32+29) /* 16-bit fp conversions */
-#define X86_FEATURE_RDRAND	( 4*32+30) /* The RDRAND instruction */
-#define X86_FEATURE_HYPERVISOR	( 4*32+31) /* Running on a hypervisor */
+#define X86_FEATURE_AES			( 4*32+25) /* AES instructions */
+#define X86_FEATURE_XSAVE		( 4*32+26) /* XSAVE/XRSTOR/XSETBV/XGETBV */
+#define X86_FEATURE_OSXSAVE		( 4*32+27) /* "" XSAVE enabled in the OS */
+#define X86_FEATURE_AVX			( 4*32+28) /* Advanced Vector Extensions */
+#define X86_FEATURE_F16C		( 4*32+29) /* 16-bit fp conversions */
+#define X86_FEATURE_RDRAND		( 4*32+30) /* The RDRAND instruction */
+#define X86_FEATURE_HYPERVISOR		( 4*32+31) /* Running on a hypervisor */
 
 /* VIA/Cyrix/Centaur-defined CPU features, CPUID level 0xC0000001, word 5 */
-#define X86_FEATURE_XSTORE	( 5*32+ 2) /* "rng" RNG present (xstore) */
-#define X86_FEATURE_XSTORE_EN	( 5*32+ 3) /* "rng_en" RNG enabled */
-#define X86_FEATURE_XCRYPT	( 5*32+ 6) /* "ace" on-CPU crypto (xcrypt) */
-#define X86_FEATURE_XCRYPT_EN	( 5*32+ 7) /* "ace_en" on-CPU crypto enabled */
-#define X86_FEATURE_ACE2	( 5*32+ 8) /* Advanced Cryptography Engine v2 */
-#define X86_FEATURE_ACE2_EN	( 5*32+ 9) /* ACE v2 enabled */
-#define X86_FEATURE_PHE		( 5*32+10) /* PadLock Hash Engine */
-#define X86_FEATURE_PHE_EN	( 5*32+11) /* PHE enabled */
-#define X86_FEATURE_PMM		( 5*32+12) /* PadLock Montgomery Multiplier */
-#define X86_FEATURE_PMM_EN	( 5*32+13) /* PMM enabled */
+#define X86_FEATURE_XSTORE		( 5*32+ 2) /* "rng" RNG present (xstore) */
+#define X86_FEATURE_XSTORE_EN		( 5*32+ 3) /* "rng_en" RNG enabled */
+#define X86_FEATURE_XCRYPT		( 5*32+ 6) /* "ace" on-CPU crypto (xcrypt) */
+#define X86_FEATURE_XCRYPT_EN		( 5*32+ 7) /* "ace_en" on-CPU crypto enabled */
+#define X86_FEATURE_ACE2		( 5*32+ 8) /* Advanced Cryptography Engine v2 */
+#define X86_FEATURE_ACE2_EN		( 5*32+ 9) /* ACE v2 enabled */
+#define X86_FEATURE_PHE			( 5*32+10) /* PadLock Hash Engine */
+#define X86_FEATURE_PHE_EN		( 5*32+11) /* PHE enabled */
+#define X86_FEATURE_PMM			( 5*32+12) /* PadLock Montgomery Multiplier */
+#define X86_FEATURE_PMM_EN		( 5*32+13) /* PMM enabled */
 
 /* More extended AMD flags: CPUID level 0x80000001, ecx, word 6 */
-#define X86_FEATURE_LAHF_LM	( 6*32+ 0) /* LAHF/SAHF in long mode */
-#define X86_FEATURE_CMP_LEGACY	( 6*32+ 1) /* If yes HyperThreading not valid */
-#define X86_FEATURE_SVM		( 6*32+ 2) /* Secure virtual machine */
-#define X86_FEATURE_EXTAPIC	( 6*32+ 3) /* Extended APIC space */
-#define X86_FEATURE_CR8_LEGACY	( 6*32+ 4) /* CR8 in 32-bit mode */
-#define X86_FEATURE_ABM		( 6*32+ 5) /* Advanced bit manipulation */
-#define X86_FEATURE_SSE4A	( 6*32+ 6) /* SSE-4A */
-#define X86_FEATURE_MISALIGNSSE ( 6*32+ 7) /* Misaligned SSE mode */
-#define X86_FEATURE_3DNOWPREFETCH ( 6*32+ 8) /* 3DNow prefetch instructions */
-#define X86_FEATURE_OSVW	( 6*32+ 9) /* OS Visible Workaround */
-#define X86_FEATURE_IBS		( 6*32+10) /* Instruction Based Sampling */
-#define X86_FEATURE_XOP		( 6*32+11) /* extended AVX instructions */
-#define X86_FEATURE_SKINIT	( 6*32+12) /* SKINIT/STGI instructions */
-#define X86_FEATURE_WDT		( 6*32+13) /* Watchdog timer */
-#define X86_FEATURE_LWP		( 6*32+15) /* Light Weight Profiling */
-#define X86_FEATURE_FMA4	( 6*32+16) /* 4 operands MAC instructions */
-#define X86_FEATURE_TCE		( 6*32+17) /* translation cache extension */
-#define X86_FEATURE_NODEID_MSR	( 6*32+19) /* NodeId MSR */
-#define X86_FEATURE_TBM		( 6*32+21) /* trailing bit manipulations */
-#define X86_FEATURE_TOPOEXT	( 6*32+22) /* topology extensions CPUID leafs */
-#define X86_FEATURE_PERFCTR_CORE ( 6*32+23) /* core performance counter extensions */
-#define X86_FEATURE_PERFCTR_NB  ( 6*32+24) /* NB performance counter extensions */
-#define X86_FEATURE_BPEXT	(6*32+26) /* data breakpoint extension */
-#define X86_FEATURE_PTSC	( 6*32+27) /* performance time-stamp counter */
-#define X86_FEATURE_PERFCTR_L2	( 6*32+28) /* L2 performance counter extensions */
-#define X86_FEATURE_MWAITX	( 6*32+29) /* MWAIT extension (MONITORX/MWAITX) */
+#define X86_FEATURE_LAHF_LM		( 6*32+ 0) /* LAHF/SAHF in long mode */
+#define X86_FEATURE_CMP_LEGACY		( 6*32+ 1) /* If yes HyperThreading not valid */
+#define X86_FEATURE_SVM			( 6*32+ 2) /* Secure virtual machine */
+#define X86_FEATURE_EXTAPIC		( 6*32+ 3) /* Extended APIC space */
+#define X86_FEATURE_CR8_LEGACY		( 6*32+ 4) /* CR8 in 32-bit mode */
+#define X86_FEATURE_ABM			( 6*32+ 5) /* Advanced bit manipulation */
+#define X86_FEATURE_SSE4A		( 6*32+ 6) /* SSE-4A */
+#define X86_FEATURE_MISALIGNSSE		( 6*32+ 7) /* Misaligned SSE mode */
+#define X86_FEATURE_3DNOWPREFETCH	( 6*32+ 8) /* 3DNow prefetch instructions */
+#define X86_FEATURE_OSVW		( 6*32+ 9) /* OS Visible Workaround */
+#define X86_FEATURE_IBS			( 6*32+10) /* Instruction Based Sampling */
+#define X86_FEATURE_XOP			( 6*32+11) /* extended AVX instructions */
+#define X86_FEATURE_SKINIT		( 6*32+12) /* SKINIT/STGI instructions */
+#define X86_FEATURE_WDT			( 6*32+13) /* Watchdog timer */
+#define X86_FEATURE_LWP			( 6*32+15) /* Light Weight Profiling */
+#define X86_FEATURE_FMA4		( 6*32+16) /* 4 operands MAC instructions */
+#define X86_FEATURE_TCE			( 6*32+17) /* translation cache extension */
+#define X86_FEATURE_NODEID_MSR		( 6*32+19) /* NodeId MSR */
+#define X86_FEATURE_TBM			( 6*32+21) /* trailing bit manipulations */
+#define X86_FEATURE_TOPOEXT		( 6*32+22) /* topology extensions CPUID leafs */
+#define X86_FEATURE_PERFCTR_CORE	( 6*32+23) /* core performance counter extensions */
+#define X86_FEATURE_PERFCTR_NB		( 6*32+24) /* NB performance counter extensions */
+#define X86_FEATURE_BPEXT		(6*32+26) /* data breakpoint extension */
+#define X86_FEATURE_PTSC		( 6*32+27) /* performance time-stamp counter */
+#define X86_FEATURE_PERFCTR_L2		( 6*32+28) /* Last Level Cache performance counter extensions */
+#define X86_FEATURE_MWAITX		( 6*32+29) /* MWAIT extension (MONITORX/MWAITX) */
 
 /*
  * Auxiliary flags: Linux defined - For features scattered in various
@@ -191,150 +191,152 @@
  *
  * Reuse free bits when adding new feature flags!
  */
-#define X86_FEATURE_RING3MWAIT	( 7*32+ 0) /* Ring 3 MONITOR/MWAIT */
-#define X86_FEATURE_CPUID_FAULT ( 7*32+ 1) /* Intel CPUID faulting */
-#define X86_FEATURE_CPB		( 7*32+ 2) /* AMD Core Performance Boost */
-#define X86_FEATURE_EPB		( 7*32+ 3) /* IA32_ENERGY_PERF_BIAS support */
-#define X86_FEATURE_CAT_L3	( 7*32+ 4) /* Cache Allocation Technology L3 */
-#define X86_FEATURE_CAT_L2	( 7*32+ 5) /* Cache Allocation Technology L2 */
-#define X86_FEATURE_CDP_L3	( 7*32+ 6) /* Code and Data Prioritization L3 */
+#define X86_FEATURE_RING3MWAIT		( 7*32+ 0) /* Ring 3 MONITOR/MWAIT */
+#define X86_FEATURE_CPUID_FAULT		( 7*32+ 1) /* Intel CPUID faulting */
+#define X86_FEATURE_CPB			( 7*32+ 2) /* AMD Core Performance Boost */
+#define X86_FEATURE_EPB			( 7*32+ 3) /* IA32_ENERGY_PERF_BIAS support */
+#define X86_FEATURE_CAT_L3		( 7*32+ 4) /* Cache Allocation Technology L3 */
+#define X86_FEATURE_CAT_L2		( 7*32+ 5) /* Cache Allocation Technology L2 */
+#define X86_FEATURE_CDP_L3		( 7*32+ 6) /* Code and Data Prioritization L3 */
 
-#define X86_FEATURE_HW_PSTATE	( 7*32+ 8) /* AMD HW-PState */
-#define X86_FEATURE_PROC_FEEDBACK ( 7*32+ 9) /* AMD ProcFeedbackInterface */
+#define X86_FEATURE_HW_PSTATE		( 7*32+ 8) /* AMD HW-PState */
+#define X86_FEATURE_PROC_FEEDBACK	( 7*32+ 9) /* AMD ProcFeedbackInterface */
+#define X86_FEATURE_SME			( 7*32+10) /* AMD Secure Memory Encryption */
 
-#define X86_FEATURE_INTEL_PPIN	( 7*32+14) /* Intel Processor Inventory Number */
-#define X86_FEATURE_INTEL_PT	( 7*32+15) /* Intel Processor Trace */
-#define X86_FEATURE_AVX512_4VNNIW (7*32+16) /* AVX-512 Neural Network Instructions */
-#define X86_FEATURE_AVX512_4FMAPS (7*32+17) /* AVX-512 Multiply Accumulation Single precision */
+#define X86_FEATURE_INTEL_PPIN		( 7*32+14) /* Intel Processor Inventory Number */
+#define X86_FEATURE_INTEL_PT		( 7*32+15) /* Intel Processor Trace */
+#define X86_FEATURE_AVX512_4VNNIW	(7*32+16) /* AVX-512 Neural Network Instructions */
+#define X86_FEATURE_AVX512_4FMAPS	(7*32+17) /* AVX-512 Multiply Accumulation Single precision */
 
-#define X86_FEATURE_MBA         ( 7*32+18) /* Memory Bandwidth Allocation */
+#define X86_FEATURE_MBA			( 7*32+18) /* Memory Bandwidth Allocation */
 
 /* Virtualization flags: Linux defined, word 8 */
-#define X86_FEATURE_TPR_SHADOW  ( 8*32+ 0) /* Intel TPR Shadow */
-#define X86_FEATURE_VNMI        ( 8*32+ 1) /* Intel Virtual NMI */
-#define X86_FEATURE_FLEXPRIORITY ( 8*32+ 2) /* Intel FlexPriority */
-#define X86_FEATURE_EPT         ( 8*32+ 3) /* Intel Extended Page Table */
-#define X86_FEATURE_VPID        ( 8*32+ 4) /* Intel Virtual Processor ID */
+#define X86_FEATURE_TPR_SHADOW		( 8*32+ 0) /* Intel TPR Shadow */
+#define X86_FEATURE_VNMI		( 8*32+ 1) /* Intel Virtual NMI */
+#define X86_FEATURE_FLEXPRIORITY	( 8*32+ 2) /* Intel FlexPriority */
+#define X86_FEATURE_EPT			( 8*32+ 3) /* Intel Extended Page Table */
+#define X86_FEATURE_VPID		( 8*32+ 4) /* Intel Virtual Processor ID */
 
-#define X86_FEATURE_VMMCALL     ( 8*32+15) /* Prefer vmmcall to vmcall */
-#define X86_FEATURE_XENPV       ( 8*32+16) /* "" Xen paravirtual guest */
+#define X86_FEATURE_VMMCALL		( 8*32+15) /* Prefer vmmcall to vmcall */
+#define X86_FEATURE_XENPV		( 8*32+16) /* "" Xen paravirtual guest */
 
 
 /* Intel-defined CPU features, CPUID level 0x00000007:0 (ebx), word 9 */
-#define X86_FEATURE_FSGSBASE	( 9*32+ 0) /* {RD/WR}{FS/GS}BASE instructions*/
-#define X86_FEATURE_TSC_ADJUST	( 9*32+ 1) /* TSC adjustment MSR 0x3b */
-#define X86_FEATURE_BMI1	( 9*32+ 3) /* 1st group bit manipulation extensions */
-#define X86_FEATURE_HLE		( 9*32+ 4) /* Hardware Lock Elision */
-#define X86_FEATURE_AVX2	( 9*32+ 5) /* AVX2 instructions */
-#define X86_FEATURE_SMEP	( 9*32+ 7) /* Supervisor Mode Execution Protection */
-#define X86_FEATURE_BMI2	( 9*32+ 8) /* 2nd group bit manipulation extensions */
-#define X86_FEATURE_ERMS	( 9*32+ 9) /* Enhanced REP MOVSB/STOSB */
-#define X86_FEATURE_INVPCID	( 9*32+10) /* Invalidate Processor Context ID */
-#define X86_FEATURE_RTM		( 9*32+11) /* Restricted Transactional Memory */
-#define X86_FEATURE_CQM		( 9*32+12) /* Cache QoS Monitoring */
-#define X86_FEATURE_MPX		( 9*32+14) /* Memory Protection Extension */
-#define X86_FEATURE_RDT_A	( 9*32+15) /* Resource Director Technology Allocation */
-#define X86_FEATURE_AVX512F	( 9*32+16) /* AVX-512 Foundation */
-#define X86_FEATURE_AVX512DQ	( 9*32+17) /* AVX-512 DQ (Double/Quad granular) Instructions */
-#define X86_FEATURE_RDSEED	( 9*32+18) /* The RDSEED instruction */
-#define X86_FEATURE_ADX		( 9*32+19) /* The ADCX and ADOX instructions */
-#define X86_FEATURE_SMAP	( 9*32+20) /* Supervisor Mode Access Prevention */
-#define X86_FEATURE_AVX512IFMA  ( 9*32+21) /* AVX-512 Integer Fused Multiply-Add instructions */
-#define X86_FEATURE_CLFLUSHOPT	( 9*32+23) /* CLFLUSHOPT instruction */
-#define X86_FEATURE_CLWB	( 9*32+24) /* CLWB instruction */
-#define X86_FEATURE_AVX512PF	( 9*32+26) /* AVX-512 Prefetch */
-#define X86_FEATURE_AVX512ER	( 9*32+27) /* AVX-512 Exponential and Reciprocal */
-#define X86_FEATURE_AVX512CD	( 9*32+28) /* AVX-512 Conflict Detection */
-#define X86_FEATURE_SHA_NI	( 9*32+29) /* SHA1/SHA256 Instruction Extensions */
-#define X86_FEATURE_AVX512BW	( 9*32+30) /* AVX-512 BW (Byte/Word granular) Instructions */
-#define X86_FEATURE_AVX512VL	( 9*32+31) /* AVX-512 VL (128/256 Vector Length) Extensions */
+#define X86_FEATURE_FSGSBASE		( 9*32+ 0) /* {RD/WR}{FS/GS}BASE instructions*/
+#define X86_FEATURE_TSC_ADJUST		( 9*32+ 1) /* TSC adjustment MSR 0x3b */
+#define X86_FEATURE_BMI1		( 9*32+ 3) /* 1st group bit manipulation extensions */
+#define X86_FEATURE_HLE			( 9*32+ 4) /* Hardware Lock Elision */
+#define X86_FEATURE_AVX2		( 9*32+ 5) /* AVX2 instructions */
+#define X86_FEATURE_SMEP		( 9*32+ 7) /* Supervisor Mode Execution Protection */
+#define X86_FEATURE_BMI2		( 9*32+ 8) /* 2nd group bit manipulation extensions */
+#define X86_FEATURE_ERMS		( 9*32+ 9) /* Enhanced REP MOVSB/STOSB */
+#define X86_FEATURE_INVPCID		( 9*32+10) /* Invalidate Processor Context ID */
+#define X86_FEATURE_RTM			( 9*32+11) /* Restricted Transactional Memory */
+#define X86_FEATURE_CQM			( 9*32+12) /* Cache QoS Monitoring */
+#define X86_FEATURE_MPX			( 9*32+14) /* Memory Protection Extension */
+#define X86_FEATURE_RDT_A		( 9*32+15) /* Resource Director Technology Allocation */
+#define X86_FEATURE_AVX512F		( 9*32+16) /* AVX-512 Foundation */
+#define X86_FEATURE_AVX512DQ		( 9*32+17) /* AVX-512 DQ (Double/Quad granular) Instructions */
+#define X86_FEATURE_RDSEED		( 9*32+18) /* The RDSEED instruction */
+#define X86_FEATURE_ADX			( 9*32+19) /* The ADCX and ADOX instructions */
+#define X86_FEATURE_SMAP		( 9*32+20) /* Supervisor Mode Access Prevention */
+#define X86_FEATURE_AVX512IFMA		( 9*32+21) /* AVX-512 Integer Fused Multiply-Add instructions */
+#define X86_FEATURE_CLFLUSHOPT		( 9*32+23) /* CLFLUSHOPT instruction */
+#define X86_FEATURE_CLWB		( 9*32+24) /* CLWB instruction */
+#define X86_FEATURE_AVX512PF		( 9*32+26) /* AVX-512 Prefetch */
+#define X86_FEATURE_AVX512ER		( 9*32+27) /* AVX-512 Exponential and Reciprocal */
+#define X86_FEATURE_AVX512CD		( 9*32+28) /* AVX-512 Conflict Detection */
+#define X86_FEATURE_SHA_NI		( 9*32+29) /* SHA1/SHA256 Instruction Extensions */
+#define X86_FEATURE_AVX512BW		( 9*32+30) /* AVX-512 BW (Byte/Word granular) Instructions */
+#define X86_FEATURE_AVX512VL		( 9*32+31) /* AVX-512 VL (128/256 Vector Length) Extensions */
 
 /* Extended state features, CPUID level 0x0000000d:1 (eax), word 10 */
-#define X86_FEATURE_XSAVEOPT	(10*32+ 0) /* XSAVEOPT */
-#define X86_FEATURE_XSAVEC	(10*32+ 1) /* XSAVEC */
-#define X86_FEATURE_XGETBV1	(10*32+ 2) /* XGETBV with ECX = 1 */
-#define X86_FEATURE_XSAVES	(10*32+ 3) /* XSAVES/XRSTORS */
+#define X86_FEATURE_XSAVEOPT		(10*32+ 0) /* XSAVEOPT */
+#define X86_FEATURE_XSAVEC		(10*32+ 1) /* XSAVEC */
+#define X86_FEATURE_XGETBV1		(10*32+ 2) /* XGETBV with ECX = 1 */
+#define X86_FEATURE_XSAVES		(10*32+ 3) /* XSAVES/XRSTORS */
 
 /* Intel-defined CPU QoS Sub-leaf, CPUID level 0x0000000F:0 (edx), word 11 */
-#define X86_FEATURE_CQM_LLC	(11*32+ 1) /* LLC QoS if 1 */
+#define X86_FEATURE_CQM_LLC		(11*32+ 1) /* LLC QoS if 1 */
 
 /* Intel-defined CPU QoS Sub-leaf, CPUID level 0x0000000F:1 (edx), word 12 */
-#define X86_FEATURE_CQM_OCCUP_LLC (12*32+ 0) /* LLC occupancy monitoring if 1 */
-#define X86_FEATURE_CQM_MBM_TOTAL (12*32+ 1) /* LLC Total MBM monitoring */
-#define X86_FEATURE_CQM_MBM_LOCAL (12*32+ 2) /* LLC Local MBM monitoring */
+#define X86_FEATURE_CQM_OCCUP_LLC	(12*32+ 0) /* LLC occupancy monitoring if 1 */
+#define X86_FEATURE_CQM_MBM_TOTAL	(12*32+ 1) /* LLC Total MBM monitoring */
+#define X86_FEATURE_CQM_MBM_LOCAL	(12*32+ 2) /* LLC Local MBM monitoring */
 
 /* AMD-defined CPU features, CPUID level 0x80000008 (ebx), word 13 */
-#define X86_FEATURE_CLZERO	(13*32+0) /* CLZERO instruction */
-#define X86_FEATURE_IRPERF	(13*32+1) /* Instructions Retired Count */
+#define X86_FEATURE_CLZERO		(13*32+0) /* CLZERO instruction */
+#define X86_FEATURE_IRPERF		(13*32+1) /* Instructions Retired Count */
 
 /* Thermal and Power Management Leaf, CPUID level 0x00000006 (eax), word 14 */
-#define X86_FEATURE_DTHERM	(14*32+ 0) /* Digital Thermal Sensor */
-#define X86_FEATURE_IDA		(14*32+ 1) /* Intel Dynamic Acceleration */
-#define X86_FEATURE_ARAT	(14*32+ 2) /* Always Running APIC Timer */
-#define X86_FEATURE_PLN		(14*32+ 4) /* Intel Power Limit Notification */
-#define X86_FEATURE_PTS		(14*32+ 6) /* Intel Package Thermal Status */
-#define X86_FEATURE_HWP		(14*32+ 7) /* Intel Hardware P-states */
-#define X86_FEATURE_HWP_NOTIFY	(14*32+ 8) /* HWP Notification */
-#define X86_FEATURE_HWP_ACT_WINDOW (14*32+ 9) /* HWP Activity Window */
-#define X86_FEATURE_HWP_EPP	(14*32+10) /* HWP Energy Perf. Preference */
-#define X86_FEATURE_HWP_PKG_REQ (14*32+11) /* HWP Package Level Request */
+#define X86_FEATURE_DTHERM		(14*32+ 0) /* Digital Thermal Sensor */
+#define X86_FEATURE_IDA			(14*32+ 1) /* Intel Dynamic Acceleration */
+#define X86_FEATURE_ARAT		(14*32+ 2) /* Always Running APIC Timer */
+#define X86_FEATURE_PLN			(14*32+ 4) /* Intel Power Limit Notification */
+#define X86_FEATURE_PTS			(14*32+ 6) /* Intel Package Thermal Status */
+#define X86_FEATURE_HWP			(14*32+ 7) /* Intel Hardware P-states */
+#define X86_FEATURE_HWP_NOTIFY		(14*32+ 8) /* HWP Notification */
+#define X86_FEATURE_HWP_ACT_WINDOW	(14*32+ 9) /* HWP Activity Window */
+#define X86_FEATURE_HWP_EPP		(14*32+10) /* HWP Energy Perf. Preference */
+#define X86_FEATURE_HWP_PKG_REQ		(14*32+11) /* HWP Package Level Request */
 
 /* AMD SVM Feature Identification, CPUID level 0x8000000a (edx), word 15 */
-#define X86_FEATURE_NPT		(15*32+ 0) /* Nested Page Table support */
-#define X86_FEATURE_LBRV	(15*32+ 1) /* LBR Virtualization support */
-#define X86_FEATURE_SVML	(15*32+ 2) /* "svm_lock" SVM locking MSR */
-#define X86_FEATURE_NRIPS	(15*32+ 3) /* "nrip_save" SVM next_rip save */
-#define X86_FEATURE_TSCRATEMSR  (15*32+ 4) /* "tsc_scale" TSC scaling support */
-#define X86_FEATURE_VMCBCLEAN   (15*32+ 5) /* "vmcb_clean" VMCB clean bits support */
-#define X86_FEATURE_FLUSHBYASID (15*32+ 6) /* flush-by-ASID support */
-#define X86_FEATURE_DECODEASSISTS (15*32+ 7) /* Decode Assists support */
-#define X86_FEATURE_PAUSEFILTER (15*32+10) /* filtered pause intercept */
-#define X86_FEATURE_PFTHRESHOLD (15*32+12) /* pause filter threshold */
-#define X86_FEATURE_AVIC	(15*32+13) /* Virtual Interrupt Controller */
-#define X86_FEATURE_V_VMSAVE_VMLOAD (15*32+15) /* Virtual VMSAVE VMLOAD */
+#define X86_FEATURE_NPT			(15*32+ 0) /* Nested Page Table support */
+#define X86_FEATURE_LBRV		(15*32+ 1) /* LBR Virtualization support */
+#define X86_FEATURE_SVML		(15*32+ 2) /* "svm_lock" SVM locking MSR */
+#define X86_FEATURE_NRIPS		(15*32+ 3) /* "nrip_save" SVM next_rip save */
+#define X86_FEATURE_TSCRATEMSR		(15*32+ 4) /* "tsc_scale" TSC scaling support */
+#define X86_FEATURE_VMCBCLEAN		(15*32+ 5) /* "vmcb_clean" VMCB clean bits support */
+#define X86_FEATURE_FLUSHBYASID		(15*32+ 6) /* flush-by-ASID support */
+#define X86_FEATURE_DECODEASSISTS	(15*32+ 7) /* Decode Assists support */
+#define X86_FEATURE_PAUSEFILTER		(15*32+10) /* filtered pause intercept */
+#define X86_FEATURE_PFTHRESHOLD		(15*32+12) /* pause filter threshold */
+#define X86_FEATURE_AVIC		(15*32+13) /* Virtual Interrupt Controller */
+#define X86_FEATURE_V_VMSAVE_VMLOAD	(15*32+15) /* Virtual VMSAVE VMLOAD */
+#define X86_FEATURE_VGIF		(15*32+16) /* Virtual GIF */
 
 /* Intel-defined CPU features, CPUID level 0x00000007:0 (ecx), word 16 */
-#define X86_FEATURE_AVX512VBMI  (16*32+ 1) /* AVX512 Vector Bit Manipulation instructions*/
-#define X86_FEATURE_PKU		(16*32+ 3) /* Protection Keys for Userspace */
-#define X86_FEATURE_OSPKE	(16*32+ 4) /* OS Protection Keys Enable */
-#define X86_FEATURE_AVX512_VBMI2 (16*32+ 6) /* Additional AVX512 Vector Bit Manipulation Instructions */
-#define X86_FEATURE_GFNI	(16*32+ 8) /* Galois Field New Instructions */
-#define X86_FEATURE_VAES	(16*32+ 9) /* Vector AES */
-#define X86_FEATURE_VPCLMULQDQ	(16*32+ 10) /* Carry-Less Multiplication Double Quadword */
-#define X86_FEATURE_AVX512_VNNI (16*32+ 11) /* Vector Neural Network Instructions */
-#define X86_FEATURE_AVX512_BITALG (16*32+12) /* Support for VPOPCNT[B,W] and VPSHUF-BITQMB */
-#define X86_FEATURE_AVX512_VPOPCNTDQ (16*32+14) /* POPCNT for vectors of DW/QW */
-#define X86_FEATURE_LA57	(16*32+16) /* 5-level page tables */
-#define X86_FEATURE_RDPID	(16*32+22) /* RDPID instruction */
+#define X86_FEATURE_AVX512VBMI		(16*32+ 1) /* AVX512 Vector Bit Manipulation instructions*/
+#define X86_FEATURE_PKU			(16*32+ 3) /* Protection Keys for Userspace */
+#define X86_FEATURE_OSPKE		(16*32+ 4) /* OS Protection Keys Enable */
+#define X86_FEATURE_AVX512_VBMI2	(16*32+ 6) /* Additional AVX512 Vector Bit Manipulation Instructions */
+#define X86_FEATURE_GFNI		(16*32+ 8) /* Galois Field New Instructions */
+#define X86_FEATURE_VAES		(16*32+ 9) /* Vector AES */
+#define X86_FEATURE_VPCLMULQDQ		(16*32+ 10) /* Carry-Less Multiplication Double Quadword */
+#define X86_FEATURE_AVX512_VNNI		(16*32+ 11) /* Vector Neural Network Instructions */
+#define X86_FEATURE_AVX512_BITALG	(16*32+12) /* Support for VPOPCNT[B,W] and VPSHUF-BITQMB */
+#define X86_FEATURE_AVX512_VPOPCNTDQ	(16*32+14) /* POPCNT for vectors of DW/QW */
+#define X86_FEATURE_LA57		(16*32+16) /* 5-level page tables */
+#define X86_FEATURE_RDPID		(16*32+22) /* RDPID instruction */
 
 /* AMD-defined CPU features, CPUID level 0x80000007 (ebx), word 17 */
-#define X86_FEATURE_OVERFLOW_RECOV (17*32+0) /* MCA overflow recovery support */
-#define X86_FEATURE_SUCCOR	(17*32+1) /* Uncorrectable error containment and recovery */
-#define X86_FEATURE_SMCA	(17*32+3) /* Scalable MCA */
+#define X86_FEATURE_OVERFLOW_RECOV	(17*32+0) /* MCA overflow recovery support */
+#define X86_FEATURE_SUCCOR		(17*32+1) /* Uncorrectable error containment and recovery */
+#define X86_FEATURE_SMCA		(17*32+3) /* Scalable MCA */
 
 /*
  * BUG word(s)
  */
-#define X86_BUG(x)		(NCAPINTS*32 + (x))
+#define X86_BUG(x)			(NCAPINTS*32 + (x))
 
-#define X86_BUG_F00F		X86_BUG(0) /* Intel F00F */
-#define X86_BUG_FDIV		X86_BUG(1) /* FPU FDIV */
-#define X86_BUG_COMA		X86_BUG(2) /* Cyrix 6x86 coma */
-#define X86_BUG_AMD_TLB_MMATCH	X86_BUG(3) /* "tlb_mmatch" AMD Erratum 383 */
-#define X86_BUG_AMD_APIC_C1E	X86_BUG(4) /* "apic_c1e" AMD Erratum 400 */
-#define X86_BUG_11AP		X86_BUG(5) /* Bad local APIC aka 11AP */
-#define X86_BUG_FXSAVE_LEAK	X86_BUG(6) /* FXSAVE leaks FOP/FIP/FOP */
-#define X86_BUG_CLFLUSH_MONITOR	X86_BUG(7) /* AAI65, CLFLUSH required before MONITOR */
-#define X86_BUG_SYSRET_SS_ATTRS	X86_BUG(8) /* SYSRET doesn't fix up SS attrs */
+#define X86_BUG_F00F			X86_BUG(0) /* Intel F00F */
+#define X86_BUG_FDIV			X86_BUG(1) /* FPU FDIV */
+#define X86_BUG_COMA			X86_BUG(2) /* Cyrix 6x86 coma */
+#define X86_BUG_AMD_TLB_MMATCH		X86_BUG(3) /* "tlb_mmatch" AMD Erratum 383 */
+#define X86_BUG_AMD_APIC_C1E		X86_BUG(4) /* "apic_c1e" AMD Erratum 400 */
+#define X86_BUG_11AP			X86_BUG(5) /* Bad local APIC aka 11AP */
+#define X86_BUG_FXSAVE_LEAK		X86_BUG(6) /* FXSAVE leaks FOP/FIP/FOP */
+#define X86_BUG_CLFLUSH_MONITOR		X86_BUG(7) /* AAI65, CLFLUSH required before MONITOR */
+#define X86_BUG_SYSRET_SS_ATTRS		X86_BUG(8) /* SYSRET doesn't fix up SS attrs */
 #ifdef CONFIG_X86_32
 /*
  * 64-bit kernels don't use X86_BUG_ESPFIX.  Make the define conditional
  * to avoid confusion.
  */
-#define X86_BUG_ESPFIX		X86_BUG(9) /* "" IRET to 16-bit SS corrupts ESP/RSP high bits */
+#define X86_BUG_ESPFIX			X86_BUG(9) /* "" IRET to 16-bit SS corrupts ESP/RSP high bits */
 #endif
-#define X86_BUG_NULL_SEG	X86_BUG(10) /* Nulling a selector preserves the base */
-#define X86_BUG_SWAPGS_FENCE	X86_BUG(11) /* SWAPGS without input dep on GS */
-#define X86_BUG_MONITOR		X86_BUG(12) /* IPI required to wake up remote CPU */
-#define X86_BUG_AMD_E400	X86_BUG(13) /* CPU is among the affected by Erratum 400 */
+#define X86_BUG_NULL_SEG		X86_BUG(10) /* Nulling a selector preserves the base */
+#define X86_BUG_SWAPGS_FENCE		X86_BUG(11) /* SWAPGS without input dep on GS */
+#define X86_BUG_MONITOR			X86_BUG(12) /* IPI required to wake up remote CPU */
+#define X86_BUG_AMD_E400		X86_BUG(13) /* CPU is among the affected by Erratum 400 */
 #endif /* _ASM_X86_CPUFEATURES_H */
-- 
2.14.2

