From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Thomas Gleixner <tglx@linutronix.de>
Date: Wed, 3 Jan 2018 19:52:04 +0100
Subject: [PATCH] x86/pti: Switch to kernel CR3 at early in
 entry_SYSCALL_compat()
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

CVE-2017-5754

The preparation for PTI which added CR3 switching to the entry code
misplaced the CR3 switch in entry_SYSCALL_compat().

With PTI enabled the entry code tries to access a per cpu variable after
switching to kernel GS. This fails because that variable is not mapped to
user space. This results in a double fault and in the worst case a kernel
crash.

Move the switch ahead of the access and clobber RSP which has been saved
already.

Fixes: 8a09317b895f ("x86/mm/pti: Prepare the x86/entry assembly code for entry/exit CR3 switching")
Reported-by: Lars Wendler <wendler.lars@web.de>
Reported-by: Laura Abbott <labbott@redhat.com>
Signed-off-by: Thomas Gleixner <tglx@linutronix.de>
Cc: Borislav Betkov <bp@alien8.de>
Cc: Andy Lutomirski <luto@kernel.org>,
Cc: Dave Hansen <dave.hansen@linux.intel.com>,
Cc: Peter Zijlstra <peterz@infradead.org>,
Cc: Greg KH <gregkh@linuxfoundation.org>, ,
Cc: Boris Ostrovsky <boris.ostrovsky@oracle.com>,
Cc: Juergen Gross <jgross@suse.com>
Cc: stable@vger.kernel.org
Link: https://lkml.kernel.org/r/alpine.DEB.2.20.1801031949200.1957@nanos
Signed-off-by: Andy Whitcroft <apw@canonical.com>
Signed-off-by: Kleber Sacilotto de Souza <kleber.souza@canonical.com>
(cherry picked from commit 2f45cd7a57da0a4d7f3a91a5f577c76b9ed9eb8a)
Signed-off-by: Fabian Grünbichler <f.gruenbichler@proxmox.com>
---
 arch/x86/entry/entry_64_compat.S | 13 ++++++-------
 1 file changed, 6 insertions(+), 7 deletions(-)

diff --git a/arch/x86/entry/entry_64_compat.S b/arch/x86/entry/entry_64_compat.S
index 973527e34887..2b5e7685823c 100644
--- a/arch/x86/entry/entry_64_compat.S
+++ b/arch/x86/entry/entry_64_compat.S
@@ -189,8 +189,13 @@ ENTRY(entry_SYSCALL_compat)
 	/* Interrupts are off on entry. */
 	swapgs
 
-	/* Stash user ESP and switch to the kernel stack. */
+	/* Stash user ESP.*/
 	movl	%esp, %r8d
+
+	/* Use %rsp as scratch reg. User ESP is stashed in r8 */
+	SWITCH_TO_KERNEL_CR3 scratch_reg=%rsp
+
+	/* Switch to the kernel stack */
 	movq	PER_CPU_VAR(cpu_current_top_of_stack), %rsp
 
 	/* Construct struct pt_regs on stack */
@@ -218,12 +223,6 @@ GLOBAL(entry_SYSCALL_compat_after_hwframe)
 	pushq   $0			/* pt_regs->r14 = 0 */
 	pushq   $0			/* pt_regs->r15 = 0 */
 
-	/*
-	 * We just saved %rdi so it is safe to clobber.  It is not
-	 * preserved during the C calls inside TRACE_IRQS_OFF anyway.
-	 */
-	SWITCH_TO_KERNEL_CR3 scratch_reg=%rdi
-
 	/*
 	 * User mode is traced as though IRQs are on, and SYSENTER
 	 * turned them off.
-- 
2.14.2

