From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Peter Zijlstra <peterz@infradead.org>
Date: Thu, 4 Jan 2018 18:07:12 +0100
Subject: [PATCH] x86/events/intel/ds: Use the proper cache flush method for
 mapping ds buffers
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

commit 42f3bdc5dd962a5958bc024c1e1444248a6b8b4a upstream.

Thomas reported the following warning:

 BUG: using smp_processor_id() in preemptible [00000000] code: ovsdb-server/4498
 caller is native_flush_tlb_single+0x57/0xc0
 native_flush_tlb_single+0x57/0xc0
 __set_pte_vaddr+0x2d/0x40
 set_pte_vaddr+0x2f/0x40
 cea_set_pte+0x30/0x40
 ds_update_cea.constprop.4+0x4d/0x70
 reserve_ds_buffers+0x159/0x410
 x86_reserve_hardware+0x150/0x160
 x86_pmu_event_init+0x3e/0x1f0
 perf_try_init_event+0x69/0x80
 perf_event_alloc+0x652/0x740
 SyS_perf_event_open+0x3f6/0xd60
 do_syscall_64+0x5c/0x190

set_pte_vaddr is used to map the ds buffers into the cpu entry area, but
there are two problems with that:

 1) The resulting flush is not supposed to be called in preemptible context

 2) The cpu entry area is supposed to be per CPU, but the debug store
    buffers are mapped for all CPUs so these mappings need to be flushed
    globally.

Add the necessary preemption protection across the mapping code and flush
TLBs globally.

Fixes: c1961a4631da ("x86/events/intel/ds: Map debug buffers in cpu_entry_area")
Reported-by: Thomas Zeitlhofer <thomas.zeitlhofer+lkml@ze-it.at>
Signed-off-by: Peter Zijlstra <peterz@infradead.org>
Signed-off-by: Thomas Gleixner <tglx@linutronix.de>
Tested-by: Thomas Zeitlhofer <thomas.zeitlhofer+lkml@ze-it.at>
Cc: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
Cc: Hugh Dickins <hughd@google.com>
Link: https://lkml.kernel.org/r/20180104170712.GB3040@hirez.programming.kicks-ass.net
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
Signed-off-by: Fabian Grünbichler <f.gruenbichler@proxmox.com>
---
 arch/x86/events/intel/ds.c | 16 ++++++++++++++++
 1 file changed, 16 insertions(+)

diff --git a/arch/x86/events/intel/ds.c b/arch/x86/events/intel/ds.c
index 85df1f12c49e..1d236666ee0e 100644
--- a/arch/x86/events/intel/ds.c
+++ b/arch/x86/events/intel/ds.c
@@ -4,6 +4,7 @@
 
 #include <asm/cpu_entry_area.h>
 #include <asm/perf_event.h>
+#include <asm/tlbflush.h>
 #include <asm/insn.h>
 
 #include "../perf_event.h"
@@ -282,20 +283,35 @@ static DEFINE_PER_CPU(void *, insn_buffer);
 
 static void ds_update_cea(void *cea, void *addr, size_t size, pgprot_t prot)
 {
+	unsigned long start = (unsigned long)cea;
 	phys_addr_t pa;
 	size_t msz = 0;
 
 	pa = virt_to_phys(addr);
+
+	preempt_disable();
 	for (; msz < size; msz += PAGE_SIZE, pa += PAGE_SIZE, cea += PAGE_SIZE)
 		cea_set_pte(cea, pa, prot);
+
+	/*
+	 * This is a cross-CPU update of the cpu_entry_area, we must shoot down
+	 * all TLB entries for it.
+	 */
+	flush_tlb_kernel_range(start, start + size);
+	preempt_enable();
 }
 
 static void ds_clear_cea(void *cea, size_t size)
 {
+	unsigned long start = (unsigned long)cea;
 	size_t msz = 0;
 
+	preempt_disable();
 	for (; msz < size; msz += PAGE_SIZE, cea += PAGE_SIZE)
 		cea_set_pte(cea, 0, PAGE_NONE);
+
+	flush_tlb_kernel_range(start, start + size);
+	preempt_enable();
 }
 
 static void *dsalloc_pages(size_t size, gfp_t flags, int cpu)
-- 
2.14.2

