From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Thomas Gleixner <tglx@linutronix.de>
Date: Mon, 4 Dec 2017 15:07:49 +0100
Subject: [PATCH] x86/cpu_entry_area: Add debugstore entries to cpu_entry_area
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

CVE-2017-5754

The Intel PEBS/BTS debug store is a design trainwreck as it expects virtual
addresses which must be visible in any execution context.

So it is required to make these mappings visible to user space when kernel
page table isolation is active.

Provide enough room for the buffer mappings in the cpu_entry_area so the
buffers are available in the user space visible page tables.

At the point where the kernel side entry area is populated there is no
buffer available yet, but the kernel PMD must be populated. To achieve this
set the entries for these buffers to non present.

Signed-off-by: Thomas Gleixner <tglx@linutronix.de>
Cc: Andy Lutomirski <luto@kernel.org>
Cc: Boris Ostrovsky <boris.ostrovsky@oracle.com>
Cc: Borislav Petkov <bp@alien8.de>
Cc: Brian Gerst <brgerst@gmail.com>
Cc: Dave Hansen <dave.hansen@linux.intel.com>
Cc: David Laight <David.Laight@aculab.com>
Cc: Denys Vlasenko <dvlasenk@redhat.com>
Cc: Eduardo Valentin <eduval@amazon.com>
Cc: Greg KH <gregkh@linuxfoundation.org>
Cc: H. Peter Anvin <hpa@zytor.com>
Cc: Josh Poimboeuf <jpoimboe@redhat.com>
Cc: Juergen Gross <jgross@suse.com>
Cc: Linus Torvalds <torvalds@linux-foundation.org>
Cc: Peter Zijlstra <peterz@infradead.org>
Cc: Will Deacon <will.deacon@arm.com>
Cc: aliguori@amazon.com
Cc: daniel.gruss@iaik.tugraz.at
Cc: hughd@google.com
Cc: keescook@google.com
Signed-off-by: Ingo Molnar <mingo@kernel.org>
(cherry picked from commit 10043e02db7f8a4161f76434931051e7d797a5f6)
Signed-off-by: Andy Whitcroft <apw@canonical.com>
Signed-off-by: Kleber Sacilotto de Souza <kleber.souza@canonical.com>
(cherry picked from commit 4b9996f9c2d35d23a9fa2afe4f161402e6f28309)
Signed-off-by: Fabian Grünbichler <f.gruenbichler@proxmox.com>
---
 arch/x86/events/perf_event.h          | 21 ++------------------
 arch/x86/include/asm/cpu_entry_area.h | 13 +++++++++++++
 arch/x86/include/asm/intel_ds.h       | 36 +++++++++++++++++++++++++++++++++++
 arch/x86/events/intel/ds.c            |  5 +++--
 arch/x86/mm/cpu_entry_area.c          | 27 ++++++++++++++++++++++++++
 5 files changed, 81 insertions(+), 21 deletions(-)
 create mode 100644 arch/x86/include/asm/intel_ds.h

diff --git a/arch/x86/events/perf_event.h b/arch/x86/events/perf_event.h
index 590eaf7c2c3e..308bc14f58af 100644
--- a/arch/x86/events/perf_event.h
+++ b/arch/x86/events/perf_event.h
@@ -14,6 +14,8 @@
 
 #include <linux/perf_event.h>
 
+#include <asm/intel_ds.h>
+
 /* To enable MSR tracing please use the generic trace points. */
 
 /*
@@ -77,8 +79,6 @@ struct amd_nb {
 	struct event_constraint event_constraints[X86_PMC_IDX_MAX];
 };
 
-/* The maximal number of PEBS events: */
-#define MAX_PEBS_EVENTS		8
 #define PEBS_COUNTER_MASK	((1ULL << MAX_PEBS_EVENTS) - 1)
 
 /*
@@ -95,23 +95,6 @@ struct amd_nb {
 	PERF_SAMPLE_TRANSACTION | \
 	PERF_SAMPLE_REGS_INTR | PERF_SAMPLE_REGS_USER)
 
-/*
- * A debug store configuration.
- *
- * We only support architectures that use 64bit fields.
- */
-struct debug_store {
-	u64	bts_buffer_base;
-	u64	bts_index;
-	u64	bts_absolute_maximum;
-	u64	bts_interrupt_threshold;
-	u64	pebs_buffer_base;
-	u64	pebs_index;
-	u64	pebs_absolute_maximum;
-	u64	pebs_interrupt_threshold;
-	u64	pebs_event_reset[MAX_PEBS_EVENTS];
-};
-
 #define PEBS_REGS \
 	(PERF_REG_X86_AX | \
 	 PERF_REG_X86_BX | \
diff --git a/arch/x86/include/asm/cpu_entry_area.h b/arch/x86/include/asm/cpu_entry_area.h
index 2fbc69a0916e..4a7884b8dca5 100644
--- a/arch/x86/include/asm/cpu_entry_area.h
+++ b/arch/x86/include/asm/cpu_entry_area.h
@@ -5,6 +5,7 @@
 
 #include <linux/percpu-defs.h>
 #include <asm/processor.h>
+#include <asm/intel_ds.h>
 
 /*
  * cpu_entry_area is a percpu region that contains things needed by the CPU
@@ -40,6 +41,18 @@ struct cpu_entry_area {
 	 */
 	char exception_stacks[(N_EXCEPTION_STACKS - 1) * EXCEPTION_STKSZ + DEBUG_STKSZ];
 #endif
+#ifdef CONFIG_CPU_SUP_INTEL
+	/*
+	 * Per CPU debug store for Intel performance monitoring. Wastes a
+	 * full page at the moment.
+	 */
+	struct debug_store cpu_debug_store;
+	/*
+	 * The actual PEBS/BTS buffers must be mapped to user space
+	 * Reserve enough fixmap PTEs.
+	 */
+	struct debug_store_buffers cpu_debug_buffers;
+#endif
 };
 
 #define CPU_ENTRY_AREA_SIZE	(sizeof(struct cpu_entry_area))
diff --git a/arch/x86/include/asm/intel_ds.h b/arch/x86/include/asm/intel_ds.h
new file mode 100644
index 000000000000..62a9f4966b42
--- /dev/null
+++ b/arch/x86/include/asm/intel_ds.h
@@ -0,0 +1,36 @@
+#ifndef _ASM_INTEL_DS_H
+#define _ASM_INTEL_DS_H
+
+#include <linux/percpu-defs.h>
+
+#define BTS_BUFFER_SIZE		(PAGE_SIZE << 4)
+#define PEBS_BUFFER_SIZE	(PAGE_SIZE << 4)
+
+/* The maximal number of PEBS events: */
+#define MAX_PEBS_EVENTS		8
+
+/*
+ * A debug store configuration.
+ *
+ * We only support architectures that use 64bit fields.
+ */
+struct debug_store {
+	u64	bts_buffer_base;
+	u64	bts_index;
+	u64	bts_absolute_maximum;
+	u64	bts_interrupt_threshold;
+	u64	pebs_buffer_base;
+	u64	pebs_index;
+	u64	pebs_absolute_maximum;
+	u64	pebs_interrupt_threshold;
+	u64	pebs_event_reset[MAX_PEBS_EVENTS];
+} __aligned(PAGE_SIZE);
+
+DECLARE_PER_CPU_PAGE_ALIGNED(struct debug_store, cpu_debug_store);
+
+struct debug_store_buffers {
+	char	bts_buffer[BTS_BUFFER_SIZE];
+	char	pebs_buffer[PEBS_BUFFER_SIZE];
+};
+
+#endif
diff --git a/arch/x86/events/intel/ds.c b/arch/x86/events/intel/ds.c
index 98e36e0c791c..21a4ed789ec0 100644
--- a/arch/x86/events/intel/ds.c
+++ b/arch/x86/events/intel/ds.c
@@ -7,11 +7,12 @@
 
 #include "../perf_event.h"
 
+/* Waste a full page so it can be mapped into the cpu_entry_area */
+DEFINE_PER_CPU_PAGE_ALIGNED(struct debug_store, cpu_debug_store);
+
 /* The size of a BTS record in bytes: */
 #define BTS_RECORD_SIZE		24
 
-#define BTS_BUFFER_SIZE		(PAGE_SIZE << 4)
-#define PEBS_BUFFER_SIZE	(PAGE_SIZE << 4)
 #define PEBS_FIXUP_SIZE		PAGE_SIZE
 
 /*
diff --git a/arch/x86/mm/cpu_entry_area.c b/arch/x86/mm/cpu_entry_area.c
index fe814fd5e014..b9283cc27622 100644
--- a/arch/x86/mm/cpu_entry_area.c
+++ b/arch/x86/mm/cpu_entry_area.c
@@ -38,6 +38,32 @@ cea_map_percpu_pages(void *cea_vaddr, void *ptr, int pages, pgprot_t prot)
 		cea_set_pte(cea_vaddr, per_cpu_ptr_to_phys(ptr), prot);
 }
 
+static void percpu_setup_debug_store(int cpu)
+{
+#ifdef CONFIG_CPU_SUP_INTEL
+	int npages;
+	void *cea;
+
+	if (boot_cpu_data.x86_vendor != X86_VENDOR_INTEL)
+		return;
+
+	cea = &get_cpu_entry_area(cpu)->cpu_debug_store;
+	npages = sizeof(struct debug_store) / PAGE_SIZE;
+	BUILD_BUG_ON(sizeof(struct debug_store) % PAGE_SIZE != 0);
+	cea_map_percpu_pages(cea, &per_cpu(cpu_debug_store, cpu), npages,
+			     PAGE_KERNEL);
+
+	cea = &get_cpu_entry_area(cpu)->cpu_debug_buffers;
+	/*
+	 * Force the population of PMDs for not yet allocated per cpu
+	 * memory like debug store buffers.
+	 */
+	npages = sizeof(struct debug_store_buffers) / PAGE_SIZE;
+	for (; npages; npages--, cea += PAGE_SIZE)
+		cea_set_pte(cea, 0, PAGE_NONE);
+#endif
+}
+
 /* Setup the fixmap mappings only once per-processor */
 static void __init setup_cpu_entry_area(int cpu)
 {
@@ -109,6 +135,7 @@ static void __init setup_cpu_entry_area(int cpu)
 	cea_set_pte(&get_cpu_entry_area(cpu)->entry_trampoline,
 		     __pa_symbol(_entry_trampoline), PAGE_KERNEL_RX);
 #endif
+	percpu_setup_debug_store(cpu);
 }
 
 static __init void setup_cpu_entry_area_ptes(void)
-- 
2.14.2

