From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Thomas Gleixner <tglx@linutronix.de>
Date: Sat, 30 Dec 2017 22:13:54 +0100
Subject: [PATCH] x86/mm: Remove preempt_disable/enable() from
 __native_flush_tlb()
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

CVE-2017-5754

The preempt_disable/enable() pair in __native_flush_tlb() was added in
commit:

  5cf0791da5c1 ("x86/mm: Disable preemption during CR3 read+write")

... to protect the UP variant of flush_tlb_mm_range().

That preempt_disable/enable() pair should have been added to the UP variant
of flush_tlb_mm_range() instead.

The UP variant was removed with commit:

  ce4a4e565f52 ("x86/mm: Remove the UP asm/tlbflush.h code, always use the (formerly) SMP code")

... but the preempt_disable/enable() pair stayed around.

The latest change to __native_flush_tlb() in commit:

  6fd166aae78c ("x86/mm: Use/Fix PCID to optimize user/kernel switches")

... added an access to a per CPU variable outside the preempt disabled
regions, which makes no sense at all. __native_flush_tlb() must always
be called with at least preemption disabled.

Remove the preempt_disable/enable() pair and add a WARN_ON_ONCE() to catch
bad callers independent of the smp_processor_id() debugging.

Signed-off-by: Thomas Gleixner <tglx@linutronix.de>
Cc: <stable@vger.kernel.org>
Cc: Andy Lutomirski <luto@kernel.org>
Cc: Borislav Petkov <bp@alien8.de>
Cc: Dave Hansen <dave.hansen@linux.intel.com>
Cc: Dominik Brodowski <linux@dominikbrodowski.net>
Cc: Linus Torvalds <torvalds@linux-foundation.org>
Cc: Linus Torvalds <torvalds@linuxfoundation.org>
Cc: Peter Zijlstra <peterz@infradead.org>
Link: http://lkml.kernel.org/r/20171230211829.679325424@linutronix.de
Signed-off-by: Ingo Molnar <mingo@kernel.org>
(cherry picked from commit decab0888e6e14e11d53cefa85f8b3d3b45ce73c)
Signed-off-by: Andy Whitcroft <apw@canonical.com>
Signed-off-by: Kleber Sacilotto de Souza <kleber.souza@canonical.com>
(cherry picked from commit cfcf931c425b60d0092bcb4a4deb1f5d5db0e293)
Signed-off-by: Fabian Grünbichler <f.gruenbichler@proxmox.com>
---
 arch/x86/include/asm/tlbflush.h | 14 ++++++++------
 1 file changed, 8 insertions(+), 6 deletions(-)

diff --git a/arch/x86/include/asm/tlbflush.h b/arch/x86/include/asm/tlbflush.h
index 7a04a1f1ca11..ff6a6d668c32 100644
--- a/arch/x86/include/asm/tlbflush.h
+++ b/arch/x86/include/asm/tlbflush.h
@@ -334,15 +334,17 @@ static inline void invalidate_user_asid(u16 asid)
  */
 static inline void __native_flush_tlb(void)
 {
-	invalidate_user_asid(this_cpu_read(cpu_tlbstate.loaded_mm_asid));
 	/*
-	 * If current->mm == NULL then we borrow a mm which may change
-	 * during a task switch and therefore we must not be preempted
-	 * while we write CR3 back:
+	 * Preemption or interrupts must be disabled to protect the access
+	 * to the per CPU variable and to prevent being preempted between
+	 * read_cr3() and write_cr3().
 	 */
-	preempt_disable();
+	WARN_ON_ONCE(preemptible());
+
+	invalidate_user_asid(this_cpu_read(cpu_tlbstate.loaded_mm_asid));
+
+	/* If current->mm == NULL then the read_cr3() "borrows" an mm */
 	native_write_cr3(__native_read_cr3());
-	preempt_enable();
 }
 
 /*
-- 
2.14.2

