From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Dave Hansen <dave.hansen@linux.intel.com>
Date: Mon, 4 Dec 2017 15:07:39 +0100
Subject: [PATCH] x86/mm/pti: Allocate a separate user PGD
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

CVE-2017-5754

Kernel page table isolation requires to have two PGDs. One for the kernel,
which contains the full kernel mapping plus the user space mapping and one
for user space which contains the user space mappings and the minimal set
of kernel mappings which are required by the architecture to be able to
transition from and to user space.

Add the necessary preliminaries.

[ tglx: Split out from the big kaiser dump. EFI fixup from Kirill ]

Signed-off-by: Dave Hansen <dave.hansen@linux.intel.com>
Signed-off-by: Thomas Gleixner <tglx@linutronix.de>
Reviewed-by: Borislav Petkov <bp@suse.de>
Cc: Andy Lutomirski <luto@kernel.org>
Cc: Boris Ostrovsky <boris.ostrovsky@oracle.com>
Cc: Borislav Petkov <bp@alien8.de>
Cc: Brian Gerst <brgerst@gmail.com>
Cc: David Laight <David.Laight@aculab.com>
Cc: Denys Vlasenko <dvlasenk@redhat.com>
Cc: Eduardo Valentin <eduval@amazon.com>
Cc: Greg KH <gregkh@linuxfoundation.org>
Cc: H. Peter Anvin <hpa@zytor.com>
Cc: Josh Poimboeuf <jpoimboe@redhat.com>
Cc: Juergen Gross <jgross@suse.com>
Cc: Linus Torvalds <torvalds@linux-foundation.org>
Cc: Peter Zijlstra <peterz@infradead.org>
Cc: Will Deacon <will.deacon@arm.com>
Cc: aliguori@amazon.com
Cc: daniel.gruss@iaik.tugraz.at
Cc: hughd@google.com
Cc: keescook@google.com
Signed-off-by: Ingo Molnar <mingo@kernel.org>
(backported from commit d9e9a6418065bb376e5de8d93ce346939b9a37a6)
Signed-off-by: Andy Whitcroft <apw@canonical.com>
Signed-off-by: Kleber Sacilotto de Souza <kleber.souza@canonical.com>
(cherry picked from commit 0bd4b34e330d8bedf90c0497dfcef2e2286c4367)
Signed-off-by: Fabian Grünbichler <f.gruenbichler@proxmox.com>
---
 arch/x86/include/asm/pgalloc.h | 11 +++++++++++
 arch/x86/mm/pgtable.c          |  5 +++--
 arch/x86/platform/efi/efi_64.c |  5 ++++-
 arch/x86/kernel/head_64.S      | 30 +++++++++++++++++++++++++++---
 4 files changed, 45 insertions(+), 6 deletions(-)

diff --git a/arch/x86/include/asm/pgalloc.h b/arch/x86/include/asm/pgalloc.h
index b2d0cd8288aa..d65b0dee7448 100644
--- a/arch/x86/include/asm/pgalloc.h
+++ b/arch/x86/include/asm/pgalloc.h
@@ -29,6 +29,17 @@ static inline void paravirt_release_p4d(unsigned long pfn) {}
  */
 extern gfp_t __userpte_alloc_gfp;
 
+#ifdef CONFIG_PAGE_TABLE_ISOLATION
+/*
+ * Instead of one PGD, we acquire two PGDs.  Being order-1, it is
+ * both 8k in size and 8k-aligned.  That lets us just flip bit 12
+ * in a pointer to swap between the two 4k halves.
+ */
+#define PGD_ALLOCATION_ORDER 1
+#else
+#define PGD_ALLOCATION_ORDER 0
+#endif
+
 /*
  * Allocate and free page tables.
  */
diff --git a/arch/x86/mm/pgtable.c b/arch/x86/mm/pgtable.c
index 942391b5b639..90d1d8f49cf6 100644
--- a/arch/x86/mm/pgtable.c
+++ b/arch/x86/mm/pgtable.c
@@ -354,14 +354,15 @@ static inline void _pgd_free(pgd_t *pgd)
 		kmem_cache_free(pgd_cache, pgd);
 }
 #else
+
 static inline pgd_t *_pgd_alloc(void)
 {
-	return (pgd_t *)__get_free_page(PGALLOC_GFP);
+	return (pgd_t *)__get_free_pages(PGALLOC_GFP, PGD_ALLOCATION_ORDER);
 }
 
 static inline void _pgd_free(pgd_t *pgd)
 {
-	free_page((unsigned long)pgd);
+	free_pages((unsigned long)pgd, PGD_ALLOCATION_ORDER);
 }
 #endif /* CONFIG_X86_PAE */
 
diff --git a/arch/x86/platform/efi/efi_64.c b/arch/x86/platform/efi/efi_64.c
index 9bf72f5bfedb..b104224d3d6c 100644
--- a/arch/x86/platform/efi/efi_64.c
+++ b/arch/x86/platform/efi/efi_64.c
@@ -194,6 +194,9 @@ static pgd_t *efi_pgd;
  * because we want to avoid inserting EFI region mappings (EFI_VA_END
  * to EFI_VA_START) into the standard kernel page tables. Everything
  * else can be shared, see efi_sync_low_kernel_mappings().
+ *
+ * We don't want the pgd on the pgd_list and cannot use pgd_alloc() for the
+ * allocation.
  */
 int __init efi_alloc_page_tables(void)
 {
@@ -206,7 +209,7 @@ int __init efi_alloc_page_tables(void)
 		return 0;
 
 	gfp_mask = GFP_KERNEL | __GFP_NOTRACK | __GFP_ZERO;
-	efi_pgd = (pgd_t *)__get_free_page(gfp_mask);
+	efi_pgd = (pgd_t *)__get_free_pages(gfp_mask, PGD_ALLOCATION_ORDER);
 	if (!efi_pgd)
 		return -ENOMEM;
 
diff --git a/arch/x86/kernel/head_64.S b/arch/x86/kernel/head_64.S
index e785734980ad..eeaaaab54b2a 100644
--- a/arch/x86/kernel/head_64.S
+++ b/arch/x86/kernel/head_64.S
@@ -324,6 +324,27 @@ GLOBAL(early_recursion_flag)
 	.balign	PAGE_SIZE; \
 GLOBAL(name)
 
+#ifdef CONFIG_PAGE_TABLE_ISOLATION
+/*
+ * Each PGD needs to be 8k long and 8k aligned.  We do not
+ * ever go out to userspace with these, so we do not
+ * strictly *need* the second page, but this allows us to
+ * have a single set_pgd() implementation that does not
+ * need to worry about whether it has 4k or 8k to work
+ * with.
+ *
+ * This ensures PGDs are 8k long:
+ */
+#define PTI_USER_PGD_FILL	512
+/* This ensures they are 8k-aligned: */
+#define NEXT_PGD_PAGE(name) \
+	.balign 2 * PAGE_SIZE; \
+GLOBAL(name)
+#else
+#define NEXT_PGD_PAGE(name) NEXT_PAGE(name)
+#define PTI_USER_PGD_FILL	0
+#endif
+
 /* Automate the creation of 1 to 1 mapping pmd entries */
 #define PMDS(START, PERM, COUNT)			\
 	i = 0 ;						\
@@ -333,13 +354,14 @@ GLOBAL(name)
 	.endr
 
 	__INITDATA
-NEXT_PAGE(early_top_pgt)
+NEXT_PGD_PAGE(early_top_pgt)
 	.fill	511,8,0
 #ifdef CONFIG_X86_5LEVEL
 	.quad	level4_kernel_pgt - __START_KERNEL_map + _PAGE_TABLE
 #else
 	.quad	level3_kernel_pgt - __START_KERNEL_map + _PAGE_TABLE
 #endif
+	.fill	PTI_USER_PGD_FILL,8,0
 
 NEXT_PAGE(early_dynamic_pgts)
 	.fill	512*EARLY_DYNAMIC_PAGE_TABLES,8,0
@@ -347,13 +369,14 @@ NEXT_PAGE(early_dynamic_pgts)
 	.data
 
 #if defined(CONFIG_XEN_PV) || defined(CONFIG_XEN_PVH)
-NEXT_PAGE(init_top_pgt)
+NEXT_PGD_PAGE(init_top_pgt)
 	.quad   level3_ident_pgt - __START_KERNEL_map + _KERNPG_TABLE
 	.org    init_top_pgt + PGD_PAGE_OFFSET*8, 0
 	.quad   level3_ident_pgt - __START_KERNEL_map + _KERNPG_TABLE
 	.org    init_top_pgt + PGD_START_KERNEL*8, 0
 	/* (2^48-(2*1024*1024*1024))/(2^39) = 511 */
 	.quad   level3_kernel_pgt - __START_KERNEL_map + _PAGE_TABLE
+	.fill	PTI_USER_PGD_FILL,8,0
 
 NEXT_PAGE(level3_ident_pgt)
 	.quad	level2_ident_pgt - __START_KERNEL_map + _KERNPG_TABLE
@@ -364,8 +387,9 @@ NEXT_PAGE(level2_ident_pgt)
 	 */
 	PMDS(0, __PAGE_KERNEL_IDENT_LARGE_EXEC, PTRS_PER_PMD)
 #else
-NEXT_PAGE(init_top_pgt)
+NEXT_PGD_PAGE(init_top_pgt)
 	.fill	512,8,0
+	.fill	PTI_USER_PGD_FILL,8,0
 #endif
 
 #ifdef CONFIG_X86_5LEVEL
-- 
2.14.2

