From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Andy Lutomirski <luto@kernel.org>
Date: Mon, 4 Dec 2017 15:07:21 +0100
Subject: [PATCH] x86/entry/64: Separate cpu_current_top_of_stack from TSS.sp0
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

CVE-2017-5754

On 64-bit kernels, we used to assume that TSS.sp0 was the current
top of stack.  With the addition of an entry trampoline, this will
no longer be the case.  Store the current top of stack in TSS.sp1,
which is otherwise unused but shares the same cacheline.

Signed-off-by: Andy Lutomirski <luto@kernel.org>
Signed-off-by: Thomas Gleixner <tglx@linutronix.de>
Reviewed-by: Thomas Gleixner <tglx@linutronix.de>
Reviewed-by: Borislav Petkov <bp@suse.de>
Cc: Boris Ostrovsky <boris.ostrovsky@oracle.com>
Cc: Borislav Petkov <bp@alien8.de>
Cc: Borislav Petkov <bpetkov@suse.de>
Cc: Brian Gerst <brgerst@gmail.com>
Cc: Dave Hansen <dave.hansen@intel.com>
Cc: Dave Hansen <dave.hansen@linux.intel.com>
Cc: David Laight <David.Laight@aculab.com>
Cc: Denys Vlasenko <dvlasenk@redhat.com>
Cc: Eduardo Valentin <eduval@amazon.com>
Cc: Greg KH <gregkh@linuxfoundation.org>
Cc: H. Peter Anvin <hpa@zytor.com>
Cc: Josh Poimboeuf <jpoimboe@redhat.com>
Cc: Juergen Gross <jgross@suse.com>
Cc: Linus Torvalds <torvalds@linux-foundation.org>
Cc: Peter Zijlstra <peterz@infradead.org>
Cc: Rik van Riel <riel@redhat.com>
Cc: Will Deacon <will.deacon@arm.com>
Cc: aliguori@amazon.com
Cc: daniel.gruss@iaik.tugraz.at
Cc: hughd@google.com
Cc: keescook@google.com
Link: https://lkml.kernel.org/r/20171204150606.050864668@linutronix.de
Signed-off-by: Ingo Molnar <mingo@kernel.org>
(cherry picked from commit 9aaefe7b59ae00605256a7d6bd1c1456432495fc)
Signed-off-by: Andy Whitcroft <apw@canonical.com>
Signed-off-by: Kleber Sacilotto de Souza <kleber.souza@canonical.com>
(cherry picked from commit 281be4ff07f7c67dc2a9c75ab24a7b9ff25544ae)
Signed-off-by: Fabian Grünbichler <f.gruenbichler@proxmox.com>
---
 arch/x86/include/asm/processor.h   | 18 +++++++++++++-----
 arch/x86/include/asm/thread_info.h |  2 +-
 arch/x86/kernel/asm-offsets_64.c   |  1 +
 arch/x86/kernel/process.c          | 10 ++++++++++
 arch/x86/kernel/process_64.c       |  1 +
 5 files changed, 26 insertions(+), 6 deletions(-)

diff --git a/arch/x86/include/asm/processor.h b/arch/x86/include/asm/processor.h
index 55885465c3a7..1bfe4bad797a 100644
--- a/arch/x86/include/asm/processor.h
+++ b/arch/x86/include/asm/processor.h
@@ -303,7 +303,13 @@ struct x86_hw_tss {
 struct x86_hw_tss {
 	u32			reserved1;
 	u64			sp0;
+
+	/*
+	 * We store cpu_current_top_of_stack in sp1 so it's always accessible.
+	 * Linux does not use ring 1, so sp1 is not otherwise needed.
+	 */
 	u64			sp1;
+
 	u64			sp2;
 	u64			reserved2;
 	u64			ist[7];
@@ -362,6 +368,8 @@ DECLARE_PER_CPU_PAGE_ALIGNED(struct tss_struct, cpu_tss);
 
 #ifdef CONFIG_X86_32
 DECLARE_PER_CPU(unsigned long, cpu_current_top_of_stack);
+#else
+#define cpu_current_top_of_stack cpu_tss.x86_tss.sp1
 #endif
 
 /*
@@ -533,12 +541,12 @@ static inline void native_swapgs(void)
 
 static inline unsigned long current_top_of_stack(void)
 {
-#ifdef CONFIG_X86_64
-	return this_cpu_read_stable(cpu_tss.x86_tss.sp0);
-#else
-	/* sp0 on x86_32 is special in and around vm86 mode. */
+	/*
+	 *  We can't read directly from tss.sp0: sp0 on x86_32 is special in
+	 *  and around vm86 mode and sp0 on x86_64 is special because of the
+	 *  entry trampoline.
+	 */
 	return this_cpu_read_stable(cpu_current_top_of_stack);
-#endif
 }
 
 static inline bool on_thread_stack(void)
diff --git a/arch/x86/include/asm/thread_info.h b/arch/x86/include/asm/thread_info.h
index ec8ef3bbb7dc..760dd8a73927 100644
--- a/arch/x86/include/asm/thread_info.h
+++ b/arch/x86/include/asm/thread_info.h
@@ -214,7 +214,7 @@ static inline int arch_within_stack_frames(const void * const stack,
 #else /* !__ASSEMBLY__ */
 
 #ifdef CONFIG_X86_64
-# define cpu_current_top_of_stack (cpu_tss + TSS_sp0)
+# define cpu_current_top_of_stack (cpu_tss + TSS_sp1)
 #endif
 
 #endif
diff --git a/arch/x86/kernel/asm-offsets_64.c b/arch/x86/kernel/asm-offsets_64.c
index c21a5315b38e..048f68ff3396 100644
--- a/arch/x86/kernel/asm-offsets_64.c
+++ b/arch/x86/kernel/asm-offsets_64.c
@@ -65,6 +65,7 @@ int main(void)
 
 	OFFSET(TSS_ist, tss_struct, x86_tss.ist);
 	OFFSET(TSS_sp0, tss_struct, x86_tss.sp0);
+	OFFSET(TSS_sp1, tss_struct, x86_tss.sp1);
 	BLANK();
 
 #ifdef CONFIG_CC_STACKPROTECTOR
diff --git a/arch/x86/kernel/process.c b/arch/x86/kernel/process.c
index aa86e810fb54..407fc37a8718 100644
--- a/arch/x86/kernel/process.c
+++ b/arch/x86/kernel/process.c
@@ -55,6 +55,16 @@ __visible DEFINE_PER_CPU_SHARED_ALIGNED(struct tss_struct, cpu_tss) = {
 		 * Poison it.
 		 */
 		.sp0 = (1UL << (BITS_PER_LONG-1)) + 1,
+
+#ifdef CONFIG_X86_64
+		/*
+		 * .sp1 is cpu_current_top_of_stack.  The init task never
+		 * runs user code, but cpu_current_top_of_stack should still
+		 * be well defined before the first context switch.
+		 */
+		.sp1 = TOP_OF_INIT_STACK,
+#endif
+
 #ifdef CONFIG_X86_32
 		.ss0 = __KERNEL_DS,
 		.ss1 = __KERNEL_CS,
diff --git a/arch/x86/kernel/process_64.c b/arch/x86/kernel/process_64.c
index 01b119bebb68..157f81816915 100644
--- a/arch/x86/kernel/process_64.c
+++ b/arch/x86/kernel/process_64.c
@@ -461,6 +461,7 @@ __switch_to(struct task_struct *prev_p, struct task_struct *next_p)
 	 * Switch the PDA and FPU contexts.
 	 */
 	this_cpu_write(current_task, next_p);
+	this_cpu_write(cpu_current_top_of_stack, task_top_of_stack(next_p));
 
 	/* Reload sp0. */
 	update_sp0(next_p);
-- 
2.14.2

