From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Gayatri Kammela <gayatri.kammela@intel.com>
Date: Mon, 30 Oct 2017 18:20:29 -0700
Subject: [PATCH] x86/cpufeatures: Enable new SSE/AVX/AVX512 CPU features
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

CVE-2017-5754

Add a few new SSE/AVX/AVX512 instruction groups/features for enumeration
in /proc/cpuinfo: AVX512_VBMI2, GFNI, VAES, VPCLMULQDQ, AVX512_VNNI,
AVX512_BITALG.

 CPUID.(EAX=7,ECX=0):ECX[bit 6]  AVX512_VBMI2
 CPUID.(EAX=7,ECX=0):ECX[bit 8]  GFNI
 CPUID.(EAX=7,ECX=0):ECX[bit 9]  VAES
 CPUID.(EAX=7,ECX=0):ECX[bit 10] VPCLMULQDQ
 CPUID.(EAX=7,ECX=0):ECX[bit 11] AVX512_VNNI
 CPUID.(EAX=7,ECX=0):ECX[bit 12] AVX512_BITALG

Detailed information of CPUID bits for these features can be found
in the Intel Architecture Instruction Set Extensions and Future Features
Programming Interface document (refer to Table 1-1. and Table 1-2.).
A copy of this document is available at
https://bugzilla.kernel.org/show_bug.cgi?id=197239

Signed-off-by: Gayatri Kammela <gayatri.kammela@intel.com>
Acked-by: Thomas Gleixner <tglx@linutronix.de>
Cc: Andi Kleen <andi.kleen@intel.com>
Cc: Fenghua Yu <fenghua.yu@intel.com>
Cc: Linus Torvalds <torvalds@linux-foundation.org>
Cc: Peter Zijlstra <peterz@infradead.org>
Cc: Ravi Shankar <ravi.v.shankar@intel.com>
Cc: Ricardo Neri <ricardo.neri@intel.com>
Cc: Yang Zhong <yang.zhong@intel.com>
Cc: bp@alien8.de
Link: http://lkml.kernel.org/r/1509412829-23380-1-git-send-email-gayatri.kammela@intel.com
Signed-off-by: Ingo Molnar <mingo@kernel.org>
(cherry picked from commit c128dbfa0f879f8ce7b79054037889b0b2240728)
Signed-off-by: Andy Whitcroft <apw@canonical.com>
Signed-off-by: Kleber Sacilotto de Souza <kleber.souza@canonical.com>
(cherry picked from commit b29eb29c5aca4708d66fa977db40c779366636a2)
Signed-off-by: Fabian Grünbichler <f.gruenbichler@proxmox.com>
---
 arch/x86/include/asm/cpufeatures.h | 6 ++++++
 arch/x86/kernel/cpu/cpuid-deps.c   | 6 ++++++
 2 files changed, 12 insertions(+)

diff --git a/arch/x86/include/asm/cpufeatures.h b/arch/x86/include/asm/cpufeatures.h
index f4e145c4b06f..c465bd6613ed 100644
--- a/arch/x86/include/asm/cpufeatures.h
+++ b/arch/x86/include/asm/cpufeatures.h
@@ -297,6 +297,12 @@
 #define X86_FEATURE_AVX512VBMI  (16*32+ 1) /* AVX512 Vector Bit Manipulation instructions*/
 #define X86_FEATURE_PKU		(16*32+ 3) /* Protection Keys for Userspace */
 #define X86_FEATURE_OSPKE	(16*32+ 4) /* OS Protection Keys Enable */
+#define X86_FEATURE_AVX512_VBMI2 (16*32+ 6) /* Additional AVX512 Vector Bit Manipulation Instructions */
+#define X86_FEATURE_GFNI	(16*32+ 8) /* Galois Field New Instructions */
+#define X86_FEATURE_VAES	(16*32+ 9) /* Vector AES */
+#define X86_FEATURE_VPCLMULQDQ	(16*32+ 10) /* Carry-Less Multiplication Double Quadword */
+#define X86_FEATURE_AVX512_VNNI (16*32+ 11) /* Vector Neural Network Instructions */
+#define X86_FEATURE_AVX512_BITALG (16*32+12) /* Support for VPOPCNT[B,W] and VPSHUF-BITQMB */
 #define X86_FEATURE_AVX512_VPOPCNTDQ (16*32+14) /* POPCNT for vectors of DW/QW */
 #define X86_FEATURE_LA57	(16*32+16) /* 5-level page tables */
 #define X86_FEATURE_RDPID	(16*32+22) /* RDPID instruction */
diff --git a/arch/x86/kernel/cpu/cpuid-deps.c b/arch/x86/kernel/cpu/cpuid-deps.c
index c1d49842a411..c21f22d836ad 100644
--- a/arch/x86/kernel/cpu/cpuid-deps.c
+++ b/arch/x86/kernel/cpu/cpuid-deps.c
@@ -50,6 +50,12 @@ const static struct cpuid_dep cpuid_deps[] = {
 	{ X86_FEATURE_AVX512BW,		X86_FEATURE_AVX512F   },
 	{ X86_FEATURE_AVX512VL,		X86_FEATURE_AVX512F   },
 	{ X86_FEATURE_AVX512VBMI,	X86_FEATURE_AVX512F   },
+	{ X86_FEATURE_AVX512_VBMI2,	X86_FEATURE_AVX512VL  },
+	{ X86_FEATURE_GFNI,		X86_FEATURE_AVX512VL  },
+	{ X86_FEATURE_VAES,		X86_FEATURE_AVX512VL  },
+	{ X86_FEATURE_VPCLMULQDQ,	X86_FEATURE_AVX512VL  },
+	{ X86_FEATURE_AVX512_VNNI,	X86_FEATURE_AVX512VL  },
+	{ X86_FEATURE_AVX512_BITALG,	X86_FEATURE_AVX512VL  },
 	{ X86_FEATURE_AVX512_4VNNIW,	X86_FEATURE_AVX512F   },
 	{ X86_FEATURE_AVX512_4FMAPS,	X86_FEATURE_AVX512F   },
 	{ X86_FEATURE_AVX512_VPOPCNTDQ, X86_FEATURE_AVX512F   },
-- 
2.14.2

