From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Ricardo Neri <ricardo.neri-calderon@linux.intel.com>
Date: Sun, 5 Nov 2017 18:27:51 -0800
Subject: [PATCH] x86/cpufeature: Add User-Mode Instruction Prevention
 definitions
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

CVE-2017-5754

[ Note, this is a Git cherry-pick of the following commit: (limited to the cpufeatures.h file)

    3522c2a6a4f3 ("x86/cpufeature: Add User-Mode Instruction Prevention definitions")

  ... for easier x86 PTI code testing and back-porting. ]

User-Mode Instruction Prevention is a security feature present in new
Intel processors that, when set, prevents the execution of a subset of
instructions if such instructions are executed in user mode (CPL > 0).
Attempting to execute such instructions causes a general protection
exception.

The subset of instructions comprises:

 * SGDT - Store Global Descriptor Table
 * SIDT - Store Interrupt Descriptor Table
 * SLDT - Store Local Descriptor Table
 * SMSW - Store Machine Status Word
 * STR  - Store Task Register

This feature is also added to the list of disabled-features to allow
a cleaner handling of build-time configuration.

Signed-off-by: Ricardo Neri <ricardo.neri-calderon@linux.intel.com>
Reviewed-by: Thomas Gleixner <tglx@linutronix.de>
Reviewed-by: Borislav Petkov <bp@suse.de>
Cc: Andrew Morton <akpm@linux-foundation.org>
Cc: Andy Lutomirski <luto@kernel.org>
Cc: Borislav Petkov <bp@alien8.de>
Cc: Brian Gerst <brgerst@gmail.com>
Cc: Chen Yucong <slaoub@gmail.com>
Cc: Chris Metcalf <cmetcalf@mellanox.com>
Cc: Dave Hansen <dave.hansen@linux.intel.com>
Cc: Denys Vlasenko <dvlasenk@redhat.com>
Cc: Fenghua Yu <fenghua.yu@intel.com>
Cc: H. Peter Anvin <hpa@zytor.com>
Cc: Huang Rui <ray.huang@amd.com>
Cc: Jiri Slaby <jslaby@suse.cz>
Cc: Jonathan Corbet <corbet@lwn.net>
Cc: Josh Poimboeuf <jpoimboe@redhat.com>
Cc: Linus Torvalds <torvalds@linux-foundation.org>
Cc: Masami Hiramatsu <mhiramat@kernel.org>
Cc: Michael S. Tsirkin <mst@redhat.com>
Cc: Paolo Bonzini <pbonzini@redhat.com>
Cc: Paul Gortmaker <paul.gortmaker@windriver.com>
Cc: Peter Zijlstra <peterz@infradead.org>
Cc: Ravi V. Shankar <ravi.v.shankar@intel.com>
Cc: Shuah Khan <shuah@kernel.org>
Cc: Tony Luck <tony.luck@intel.com>
Cc: Vlastimil Babka <vbabka@suse.cz>
Cc: ricardo.neri@intel.com
Link: http://lkml.kernel.org/r/1509935277-22138-7-git-send-email-ricardo.neri-calderon@linux.intel.com
Signed-off-by: Ingo Molnar <mingo@kernel.org>
(cherry picked from commit a8b4db562e7283a1520f9e9730297ecaab7622ea)
Signed-off-by: Andy Whitcroft <apw@canonical.com>
Signed-off-by: Kleber Sacilotto de Souza <kleber.souza@canonical.com>
(cherry picked from commit 6193ddb9de38665ba45f7f17dd9713baec3673ca)
Signed-off-by: Fabian Grünbichler <f.gruenbichler@proxmox.com>
---
 arch/x86/include/asm/cpufeatures.h | 1 +
 1 file changed, 1 insertion(+)

diff --git a/arch/x86/include/asm/cpufeatures.h b/arch/x86/include/asm/cpufeatures.h
index 6db782ed9cdb..0ea630bb3e74 100644
--- a/arch/x86/include/asm/cpufeatures.h
+++ b/arch/x86/include/asm/cpufeatures.h
@@ -295,6 +295,7 @@
 
 /* Intel-defined CPU features, CPUID level 0x00000007:0 (ECX), word 16 */
 #define X86_FEATURE_AVX512VBMI		(16*32+ 1) /* AVX512 Vector Bit Manipulation instructions*/
+#define X86_FEATURE_UMIP		(16*32+ 2) /* User Mode Instruction Protection */
 #define X86_FEATURE_PKU			(16*32+ 3) /* Protection Keys for Userspace */
 #define X86_FEATURE_OSPKE		(16*32+ 4) /* OS Protection Keys Enable */
 #define X86_FEATURE_AVX512_VBMI2	(16*32+ 6) /* Additional AVX512 Vector Bit Manipulation Instructions */
-- 
2.14.2

