From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Andy Lutomirski <luto@kernel.org>
Date: Mon, 4 Dec 2017 15:07:15 +0100
Subject: [PATCH] x86/mm/fixmap: Generalize the GDT fixmap mechanism, introduce
 struct cpu_entry_area
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

CVE-2017-5754

Currently, the GDT is an ad-hoc array of pages, one per CPU, in the
fixmap.  Generalize it to be an array of a new 'struct cpu_entry_area'
so that we can cleanly add new things to it.

Signed-off-by: Andy Lutomirski <luto@kernel.org>
Signed-off-by: Thomas Gleixner <tglx@linutronix.de>
Reviewed-by: Thomas Gleixner <tglx@linutronix.de>
Reviewed-by: Borislav Petkov <bp@suse.de>
Cc: Boris Ostrovsky <boris.ostrovsky@oracle.com>
Cc: Borislav Petkov <bp@alien8.de>
Cc: Borislav Petkov <bpetkov@suse.de>
Cc: Brian Gerst <brgerst@gmail.com>
Cc: Dave Hansen <dave.hansen@intel.com>
Cc: Dave Hansen <dave.hansen@linux.intel.com>
Cc: David Laight <David.Laight@aculab.com>
Cc: Denys Vlasenko <dvlasenk@redhat.com>
Cc: Eduardo Valentin <eduval@amazon.com>
Cc: Greg KH <gregkh@linuxfoundation.org>
Cc: H. Peter Anvin <hpa@zytor.com>
Cc: Josh Poimboeuf <jpoimboe@redhat.com>
Cc: Juergen Gross <jgross@suse.com>
Cc: Linus Torvalds <torvalds@linux-foundation.org>
Cc: Peter Zijlstra <peterz@infradead.org>
Cc: Rik van Riel <riel@redhat.com>
Cc: Will Deacon <will.deacon@arm.com>
Cc: aliguori@amazon.com
Cc: daniel.gruss@iaik.tugraz.at
Cc: hughd@google.com
Cc: keescook@google.com
Link: https://lkml.kernel.org/r/20171204150605.563271721@linutronix.de
Signed-off-by: Ingo Molnar <mingo@kernel.org>
(cherry picked from commit ef8813ab280507972bb57e4b1b502811ad4411e9)
Signed-off-by: Andy Whitcroft <apw@canonical.com>
Signed-off-by: Kleber Sacilotto de Souza <kleber.souza@canonical.com>
(cherry picked from commit b17894f1ac91491ce29946ed946a129620b7f7ac)
Signed-off-by: Fabian Grünbichler <f.gruenbichler@proxmox.com>
---
 arch/x86/include/asm/desc.h   |  9 +--------
 arch/x86/include/asm/fixmap.h | 37 +++++++++++++++++++++++++++++++++++--
 arch/x86/kernel/cpu/common.c  | 14 +++++++-------
 arch/x86/xen/mmu_pv.c         |  2 +-
 4 files changed, 44 insertions(+), 18 deletions(-)

diff --git a/arch/x86/include/asm/desc.h b/arch/x86/include/asm/desc.h
index 22ee0a93b4f7..81c9b1e8cae9 100644
--- a/arch/x86/include/asm/desc.h
+++ b/arch/x86/include/asm/desc.h
@@ -58,17 +58,10 @@ static inline struct desc_struct *get_current_gdt_rw(void)
 	return this_cpu_ptr(&gdt_page)->gdt;
 }
 
-/* Get the fixmap index for a specific processor */
-static inline unsigned int get_cpu_gdt_ro_index(int cpu)
-{
-	return FIX_GDT_REMAP_END - cpu;
-}
-
 /* Provide the fixmap address of the remapped GDT */
 static inline struct desc_struct *get_cpu_gdt_ro(int cpu)
 {
-	unsigned int idx = get_cpu_gdt_ro_index(cpu);
-	return (struct desc_struct *)__fix_to_virt(idx);
+	return (struct desc_struct *)&get_cpu_entry_area(cpu)->gdt;
 }
 
 /* Provide the current read-only GDT */
diff --git a/arch/x86/include/asm/fixmap.h b/arch/x86/include/asm/fixmap.h
index 81c2b11f50a6..8c6ed66fe957 100644
--- a/arch/x86/include/asm/fixmap.h
+++ b/arch/x86/include/asm/fixmap.h
@@ -44,6 +44,19 @@ extern unsigned long __FIXADDR_TOP;
 			 PAGE_SIZE)
 #endif
 
+/*
+ * cpu_entry_area is a percpu region in the fixmap that contains things
+ * needed by the CPU and early entry/exit code.  Real types aren't used
+ * for all fields here to avoid circular header dependencies.
+ *
+ * Every field is a virtual alias of some other allocated backing store.
+ * There is no direct allocation of a struct cpu_entry_area.
+ */
+struct cpu_entry_area {
+	char gdt[PAGE_SIZE];
+};
+
+#define CPU_ENTRY_AREA_PAGES (sizeof(struct cpu_entry_area) / PAGE_SIZE)
 
 /*
  * Here we define all the compile-time 'special' virtual
@@ -101,8 +114,8 @@ enum fixed_addresses {
 	FIX_LNW_VRTC,
 #endif
 	/* Fixmap entries to remap the GDTs, one per processor. */
-	FIX_GDT_REMAP_BEGIN,
-	FIX_GDT_REMAP_END = FIX_GDT_REMAP_BEGIN + NR_CPUS - 1,
+	FIX_CPU_ENTRY_AREA_TOP,
+	FIX_CPU_ENTRY_AREA_BOTTOM = FIX_CPU_ENTRY_AREA_TOP + (CPU_ENTRY_AREA_PAGES * NR_CPUS) - 1,
 
 #ifdef CONFIG_ACPI_APEI_GHES
 	/* Used for GHES mapping from assorted contexts */
@@ -171,5 +184,25 @@ static inline void __set_fixmap(enum fixed_addresses idx,
 void __early_set_fixmap(enum fixed_addresses idx,
 			phys_addr_t phys, pgprot_t flags);
 
+static inline unsigned int __get_cpu_entry_area_page_index(int cpu, int page)
+{
+	BUILD_BUG_ON(sizeof(struct cpu_entry_area) % PAGE_SIZE != 0);
+
+	return FIX_CPU_ENTRY_AREA_BOTTOM - cpu*CPU_ENTRY_AREA_PAGES - page;
+}
+
+#define __get_cpu_entry_area_offset_index(cpu, offset) ({		\
+	BUILD_BUG_ON(offset % PAGE_SIZE != 0);				\
+	__get_cpu_entry_area_page_index(cpu, offset / PAGE_SIZE);	\
+	})
+
+#define get_cpu_entry_area_index(cpu, field)				\
+	__get_cpu_entry_area_offset_index((cpu), offsetof(struct cpu_entry_area, field))
+
+static inline struct cpu_entry_area *get_cpu_entry_area(int cpu)
+{
+	return (struct cpu_entry_area *)__fix_to_virt(__get_cpu_entry_area_page_index(cpu, 0));
+}
+
 #endif /* !__ASSEMBLY__ */
 #endif /* _ASM_X86_FIXMAP_H */
diff --git a/arch/x86/kernel/cpu/common.c b/arch/x86/kernel/cpu/common.c
index aa97e4cd3a33..ffee73ec1af1 100644
--- a/arch/x86/kernel/cpu/common.c
+++ b/arch/x86/kernel/cpu/common.c
@@ -466,12 +466,12 @@ void load_percpu_segment(int cpu)
 	load_stack_canary_segment();
 }
 
-/* Setup the fixmap mapping only once per-processor */
-static inline void setup_fixmap_gdt(int cpu)
+/* Setup the fixmap mappings only once per-processor */
+static inline void setup_cpu_entry_area(int cpu)
 {
 #ifdef CONFIG_X86_64
 	/* On 64-bit systems, we use a read-only fixmap GDT. */
-	pgprot_t prot = PAGE_KERNEL_RO;
+	pgprot_t gdt_prot = PAGE_KERNEL_RO;
 #else
 	/*
 	 * On native 32-bit systems, the GDT cannot be read-only because
@@ -482,11 +482,11 @@ static inline void setup_fixmap_gdt(int cpu)
 	 * On Xen PV, the GDT must be read-only because the hypervisor requires
 	 * it.
 	 */
-	pgprot_t prot = boot_cpu_has(X86_FEATURE_XENPV) ?
+	pgprot_t gdt_prot = boot_cpu_has(X86_FEATURE_XENPV) ?
 		PAGE_KERNEL_RO : PAGE_KERNEL;
 #endif
 
-	__set_fixmap(get_cpu_gdt_ro_index(cpu), get_cpu_gdt_paddr(cpu), prot);
+	__set_fixmap(get_cpu_entry_area_index(cpu, gdt), get_cpu_gdt_paddr(cpu), gdt_prot);
 }
 
 /* Load the original GDT from the per-cpu structure */
@@ -1589,7 +1589,7 @@ void cpu_init(void)
 	if (is_uv_system())
 		uv_cpu_init();
 
-	setup_fixmap_gdt(cpu);
+	setup_cpu_entry_area(cpu);
 	load_fixmap_gdt(cpu);
 }
 
@@ -1650,7 +1650,7 @@ void cpu_init(void)
 
 	fpu__init_cpu();
 
-	setup_fixmap_gdt(cpu);
+	setup_cpu_entry_area(cpu);
 	load_fixmap_gdt(cpu);
 }
 #endif
diff --git a/arch/x86/xen/mmu_pv.c b/arch/x86/xen/mmu_pv.c
index 45bb2d462e44..53e65f605bdd 100644
--- a/arch/x86/xen/mmu_pv.c
+++ b/arch/x86/xen/mmu_pv.c
@@ -2297,7 +2297,7 @@ static void xen_set_fixmap(unsigned idx, phys_addr_t phys, pgprot_t prot)
 #endif
 	case FIX_TEXT_POKE0:
 	case FIX_TEXT_POKE1:
-	case FIX_GDT_REMAP_BEGIN ... FIX_GDT_REMAP_END:
+	case FIX_CPU_ENTRY_AREA_TOP ... FIX_CPU_ENTRY_AREA_BOTTOM:
 		/* All local page mappings */
 		pte = pfn_pte(phys, prot);
 		break;
-- 
2.14.2

