From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Dave Hansen <dave.hansen@linux.intel.com>
Date: Mon, 4 Dec 2017 15:07:58 +0100
Subject: [PATCH] x86/mm: Abstract switching CR3
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

CVE-2017-5754

In preparation to adding additional PCID flushing, abstract the
loading of a new ASID into CR3.

[ PeterZ: Split out from big combo patch ]

Signed-off-by: Dave Hansen <dave.hansen@linux.intel.com>
Signed-off-by: Peter Zijlstra (Intel) <peterz@infradead.org>
Signed-off-by: Thomas Gleixner <tglx@linutronix.de>
Cc: Andy Lutomirski <luto@kernel.org>
Cc: Boris Ostrovsky <boris.ostrovsky@oracle.com>
Cc: Borislav Petkov <bp@alien8.de>
Cc: Brian Gerst <brgerst@gmail.com>
Cc: David Laight <David.Laight@aculab.com>
Cc: Denys Vlasenko <dvlasenk@redhat.com>
Cc: Eduardo Valentin <eduval@amazon.com>
Cc: Greg KH <gregkh@linuxfoundation.org>
Cc: H. Peter Anvin <hpa@zytor.com>
Cc: Josh Poimboeuf <jpoimboe@redhat.com>
Cc: Juergen Gross <jgross@suse.com>
Cc: Linus Torvalds <torvalds@linux-foundation.org>
Cc: Peter Zijlstra <peterz@infradead.org>
Cc: Will Deacon <will.deacon@arm.com>
Cc: aliguori@amazon.com
Cc: daniel.gruss@iaik.tugraz.at
Cc: hughd@google.com
Cc: keescook@google.com
Signed-off-by: Ingo Molnar <mingo@kernel.org>
(cherry picked from commit 48e111982cda033fec832c6b0592c2acedd85d04)
Signed-off-by: Andy Whitcroft <apw@canonical.com>
Signed-off-by: Kleber Sacilotto de Souza <kleber.souza@canonical.com>
(cherry picked from commit 1e2affe2a79305b3a5f3ad65d3f61ad9d1f9e168)
Signed-off-by: Fabian Grünbichler <f.gruenbichler@proxmox.com>
---
 arch/x86/mm/tlb.c | 22 ++++++++++++++++++++--
 1 file changed, 20 insertions(+), 2 deletions(-)

diff --git a/arch/x86/mm/tlb.c b/arch/x86/mm/tlb.c
index ce87b69fb4e0..353f2f4e1d96 100644
--- a/arch/x86/mm/tlb.c
+++ b/arch/x86/mm/tlb.c
@@ -101,6 +101,24 @@ static void choose_new_asid(struct mm_struct *next, u64 next_tlb_gen,
 	*need_flush = true;
 }
 
+static void load_new_mm_cr3(pgd_t *pgdir, u16 new_asid, bool need_flush)
+{
+	unsigned long new_mm_cr3;
+
+	if (need_flush) {
+		new_mm_cr3 = build_cr3(pgdir, new_asid);
+	} else {
+		new_mm_cr3 = build_cr3_noflush(pgdir, new_asid);
+	}
+
+	/*
+	 * Caution: many callers of this function expect
+	 * that load_cr3() is serializing and orders TLB
+	 * fills with respect to the mm_cpumask writes.
+	 */
+	write_cr3(new_mm_cr3);
+}
+
 void leave_mm(int cpu)
 {
 	struct mm_struct *loaded_mm = this_cpu_read(cpu_tlbstate.loaded_mm);
@@ -228,7 +246,7 @@ void switch_mm_irqs_off(struct mm_struct *prev, struct mm_struct *next,
 		if (need_flush) {
 			this_cpu_write(cpu_tlbstate.ctxs[new_asid].ctx_id, next->context.ctx_id);
 			this_cpu_write(cpu_tlbstate.ctxs[new_asid].tlb_gen, next_tlb_gen);
-			write_cr3(build_cr3(next->pgd, new_asid));
+			load_new_mm_cr3(next->pgd, new_asid, true);
 
 			/*
 			 * NB: This gets called via leave_mm() in the idle path
@@ -241,7 +259,7 @@ void switch_mm_irqs_off(struct mm_struct *prev, struct mm_struct *next,
 			trace_tlb_flush_rcuidle(TLB_FLUSH_ON_TASK_SWITCH, TLB_FLUSH_ALL);
 		} else {
 			/* The new ASID is already up to date. */
-			write_cr3(build_cr3_noflush(next->pgd, new_asid));
+			load_new_mm_cr3(next->pgd, new_asid, false);
 
 			/* See above wrt _rcuidle. */
 			trace_tlb_flush_rcuidle(TLB_FLUSH_ON_TASK_SWITCH, 0);
-- 
2.14.2

